Subject: leak on wilson creek lateral
repairs to the wilson creek lateral were completed on monday afternoon
7 / 10 / 00 . upon completion of repairs hms found excessive corrosion on the
meter run and notified pumper that they would remain shut - in until the
producer replaced or repaired the meter run . once the meter run is replaced
or repaired the lateral will be purged and packed and put back into service .
if you have any questions please call me at 36449 .
thanks
gary h
- - - - - - - - - - - - - - - - - - - - - - forwarded by gary a hanks / hou / ect on 07 / 12 / 2000 10 : 00
am - - - - - - - - - - - - - - - - - - - - - - - - - - -
enron north america corp .
from : gary a hanks 07 / 10 / 2000 11 : 04 am
to : cheryl dudley / hou / ect @ ect , melissa graves / hou / ect @ ect , george
weissman / hou / ect @ ect , daren j farmer / hou / ect @ ect , pat
clynes / corp / enron @ enron , lauri a allen / hou / ect @ ect , shawna flynn / hou / ect @ ect
cc : james mckay / hou / ect @ ect , earl tisdale / hou / ect @ ect
subject : leak on wilson creek lateral
on friday , july 7 2000 , the field detected a leak on the wilson creek lateral
in wharton co . meter # 0984284 was shut in at approximately 6 : 30 pm until
repairs are completed sometime today july 10 , 2000 .
if you have any questions please call . 36449
thanks
gary h
- - - - - - - - - - - - - - - - - - - - - - forwarded by gary a hanks / hou / ect on 07 / 10 / 2000 10 : 55
am - - - - - - - - - - - - - - - - - - - - - - - - - - -
from : michael c winders 07 / 10 / 2000 06 : 13 am
to : gary a hanks / hou / ect @ ect
cc :
subject : leak on wilson creek lateral
the producer that was shut in was zevex production # 4284 - 10 they flow about
. 3 a day .