<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<packages>
<package name="P398DLP_ADXL326_PKG">
<description>ADXL326 3 axis accelerometer</description>
</package>
<package name="P398DLP_BME680_PKG">
<description>BME680 temperature, pressure, relative humidity, and volatile organic compounds sensor</description>
</package>
<package name="P398DLP_MICROSD_PKG">
<description>Adafruit microSD reader breakout board</description>
</package>
<package name="P398DLP_MCP4725_PKG">
<description>MCP44725 DAC</description>
</package>
<package name="P398DLP_DS3231_PKG">
<description>DS3231 real time clock with battery backup</description>
</package>
<package name="1X07">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X07/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X03-CLEANBIG">
</package>
<package name="1X04">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X04/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X05">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X05/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1_05X2MM">
<description>CON-M-1X5-200</description>
</package>
<package name="1X06">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X06/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X08">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X08/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X09">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X09/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X10">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X10/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X11">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X11/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X12">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X12/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="2X18">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="2X18/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="SO08">
<description>&lt;b&gt;Small Outline Package 8&lt;/b&gt;&lt;br&gt;
NS Package M08A</description>
</package>
<package name="MMSOP08">
<description>&lt;b&gt;Molded Mini Small Outline Package&lt;/b&gt; 8 - Lead (0.118" Wide)&lt;p&gt;
NS Package Number MUA08A&lt;br&gt;
Source: http://cache.national.com/ds/LM/LM386.pdf</description>
</package>
<package name="1X16">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X16/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="PT-10">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;</description>
</package>
<package name="PT-10S">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;</description>
</package>
<package name="PT-SPIN">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;</description>
</package>
<package name="B25P">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
Beckman Helitrim 25</description>
</package>
<package name="B25U">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
Beckman Helitrim 25</description>
</package>
<package name="B25V">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
Beckman Helitrim 25</description>
</package>
<package name="B25X">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
Beckman Helitrim 25</description>
</package>
<package name="B64W">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
Beckman Helitrim 64</description>
</package>
<package name="B64Y">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
Beckman Helitrim 64</description>
</package>
<package name="SP19L">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;</description>
</package>
<package name="CA6H">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
distributor Schukat</description>
</package>
<package name="CA6V">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
distributor Schukat</description>
</package>
<package name="CA9H">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
distributor Schukat</description>
</package>
<package name="CA9V">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
distributor Schukat</description>
</package>
<package name="CA14V">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
distributor Schukat</description>
</package>
<package name="CA14H">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
distributor Schukat</description>
</package>
<package name="CT6">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
Copal</description>
</package>
<package name="ECP10P">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;</description>
</package>
<package name="ECP10S">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;</description>
</package>
<package name="LI10">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
Piher</description>
</package>
<package name="LI15">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
Piher</description>
</package>
<package name="RJ6">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
Copal</description>
</package>
<package name="RJ6S">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
Copal</description>
</package>
<package name="RJ9W">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
Copal</description>
</package>
<package name="RS3">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
Copal</description>
</package>
<package name="S63P">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
Spectrol</description>
</package>
<package name="S63S">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
Spectrol</description>
</package>
<package name="S63X">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
Spectrol</description>
</package>
<package name="S64W">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
Spectrol</description>
</package>
<package name="S64Y">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
Spectrol</description>
</package>
<package name="S75H">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;</description>
</package>
<package name="S75P">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;</description>
</package>
<package name="ST10">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
Piher</description>
</package>
<package name="ST15">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
Piher</description>
</package>
<package name="SP19LKN">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;</description>
</package>
<package name="CIP20C-4MM">
<description>&lt;b&gt;Carbon Rotary Potentiometers - 20 mm size&lt;/b&gt;&lt;p&gt;
Source: Radiohm .. RAD.pdf</description>
</package>
<package name="CIP20C-6MM">
<description>&lt;b&gt;Carbon Rotary Potentiometers - 20 mm size&lt;/b&gt;&lt;p&gt;
Source: Radiohm .. RAD.pdf</description>
</package>
<package name="SM-42/43A">
<description>&lt;b&gt;COPAL ELECTRONICS SM-42/43 SURFACE MOUNT TRIMMERS&lt;/b&gt; Side adjustmet&lt;p&gt;
Source: smt-pots.pdf</description>
</package>
<package name="SM-42/43X">
<description>&lt;b&gt;COPAL ELECTRONICS SM-42/43 SURFACE MOUNT TRIMMERS&lt;/b&gt; Top adjustmet&lt;p&gt;
Source: smt-pots.pdf</description>
</package>
<package name="SM-42/43W">
<description>&lt;b&gt;COPAL ELECTRONICS SM-42/43 SURFACE MOUNT TRIMMERS&lt;/b&gt; Top adjustmet&lt;p&gt;
Source: smt-pots.pdf</description>
</package>
<package name="SM-42/43B">
<description>&lt;b&gt;COPAL ELECTRONICS SM-42/43 SURFACE MOUNT TRIMMERS&lt;/b&gt; Side adjustmet&lt;p&gt;
Source: smt-pots.pdf</description>
</package>
<package name="3223G">
<description>&lt;b&gt;3 mm SMD Trimming Potentiometer&lt;/b&gt; Side Adjust&lt;p&gt;
Source: http://www.bourns.com/data/global/PDFs/3223.PDF</description>
</package>
<package name="3223J">
<description>&lt;b&gt;3 mm SMD Trimming Potentiometer&lt;/b&gt; Side Adjust&lt;p&gt;
Source: http://www.bourns.com/data/global/PDFs/3223.PDF</description>
</package>
<package name="3223W">
<description>&lt;b&gt;3 mm SMD Trimming Potentiometer&lt;/b&gt; Top Adjust&lt;p&gt;
Source: http://www.bourns.com/data/global/PDFs/3223.PDF</description>
</package>
<package name="MEGABOX">
<description>Empty box</description>
</package>
<package name="P398DLP_MICROPHONE_PKG">
<description>Adafruit amplified electret microphone</description>
</package>
<package name="P398DLP_ULTIMATE_GPS_PKG">
<description>Adafruit "ultimate GPS" breakout board</description>
</package>
<package name="1X02">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="P398DLP_SPEAKER_PKG">
<description>0.5 watt, 8 ohm mini-metal speaker</description>
</package>
<package name="P398DLP_RCA_PCB_JACK_PKG">
<description>pushbutton</description>
</package>
<package name="P398DLP_INA219_PKG">
<description>Adafruit INA219 current/voltage sensor</description>
</package>
<package name="TO-39">
<description>&lt;h3&gt;TO-39 4-Pin PTH&lt;/h3&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/datasheets/Sensors/Temperature/SEN-09570-datasheet-3901090614M005.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;
&lt;li&gt;Pin Count: 4&lt;/li&gt;
&lt;li&gt;Diameter: 9 mm&lt;/li&gt;
&lt;/ul&gt;
&lt;p&gt;Devices Using:&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;MLX90614&lt;/li&gt;
&lt;/ul&gt;</description>
</package>
<package name="LCD-16X2-4HOLES">
<description>2x16 liquid crystal display, four mounting holes</description>
</package>
<package name="LCD-16X2-3HOLES">
</package>
<package name="LCD-20X4-4HOLES">
</package>
<package name="LCD-20X4-3HOLES">
</package>
<package name="LCD-16X2-4HOLES-BL">
</package>
<package name="P398DLP_KEYPAD_PKG">
<description>4 x 3 keypad</description>
</package>
<package name="P398DLP_5XAA_BATTERY_PKG">
<description>Adafruit 5 x AA battery pack</description>
</package>
<package name="1X02/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X18">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X01">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="P398DLP_PAM8302A_PKG">
<description>PAM8302A pulse width modulation audio amplifier</description>
</package>
<package name="P398DLP_TSL2561_PKG">
<description>TSL2561 Lux sensor breakout board</description>
</package>
<package name="P398DLP_GUVA_ANALOG_UV_PKG">
<description>GUVA analog UV sensor</description>
</package>
<package name="P398DLP_ARDUINO_FLIPPED_PKG">
<description>Arduino MEGA 2560, components down</description>
</package>
<package name="P398DLP_VL53L0X_PKG">
<description>VL53L0X proximity sensor</description>
</package>
<package name="P398DLP_L3GD20H_PKG">
<description>L3GD20 3-Axis Gyro</description>
</package>
<package name="P398DLP_ON-OFF-ON-OFF_SWITCH_PKG">
<description>on-off-on-off pushbutton switch</description>
</package>
<package name="P398DLP_LCD_16X2_PKG">
<description>2x16 liquid crystal display, four mounting holes. Crystalfontz CFAH1602B-NGG-JTV</description>
</package>
<package name="P398DLP_TRIMPOT_PKG">
<description>trimpot</description>
</package>
<package name="P398DLP_MLX90614_IR_PKG">
<description>&lt;h3&gt;TO-39 4-Pin PTH&lt;/h3&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/datasheets/Sensors/Temperature/SEN-09570-datasheet-3901090614M005.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;
&lt;li&gt;Pin Count: 4&lt;/li&gt;
&lt;li&gt;Diameter: 9 mm&lt;/li&gt;
&lt;/ul&gt;
&lt;p&gt;Devices Using:&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;MLX90614&lt;/li&gt;
&lt;/ul&gt;</description>
</package>
<package name="P398DLP_LSM9DS1_9DOF_PKG">
<description>LSM9DS1 accelerometer, gyroscope, magnetometer</description>
</package>
<package name="P398DLP_MMA8451_ACCEL_PKG">
<description>DS3231 real time clock with battery backup</description>
</package>
<package name="P398DLP_FORCE_SENSITIVE_RESISTOR_PKG">
<description>force sensitive resistor</description>
</package>
<package name="P398DLP_ANEMOMETER_PKG">
<description>anemometer</description>
</package>
<package name="P398DLP_MYOWARE_PKG">
<description>myoware EMG sensor</description>
</package>
<package name="P398DLP_GP2Y0A21YK0F_IR_PROXIMITY_PKG">
<description>IR proximity sensor</description>
</package>
<package name="P398DLP_POWER+ADC_PKG">
<description>ADC + power + ground</description>
</package>
<package name="P398DLP_PMS5003_PM2.5_PKG">
<description>PMS5003 airborne particulates sensor</description>
</package>
<package name="P398DLP_TCA9548A_MUX_PKG">
<description>TCA9548A I2C MUX</description>
</package>
<package name="P398DLP_DRV2605L_HAPTIC_PKG">
<description>DRV2605L haptic (vibrator) driver</description>
</package>
<package name="P398DLP_HAPTIC_VIBRATOR_MOTOR_PKG">
<description>haptic vibrator</description>
</package>
<package name="P398DLP_POWER+I2C_PKG">
<description>powered off-board I2C connection</description>
</package>
<package name="P398DLP_GPPS_ANTENNA_ADAPTER_JACK_PKG">
</package>
<package name="P398DLP_M0_ADALOGGER_PKG">
</package>
<package name="P398DLP_ADALOGGER_M0_PKG">
<description>Adafruit M0 Adalogger</description>
</package>
<package name="P398DLP_74HC157N_PKG">
</package>
<package name="DIL16">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="P398DLP_PUSHBUTTON2_PKG">
<description>Adafruit tactile pushbutton, normally open</description>
</package>
<package name="P398DLP_1XAAA_BATTERY_HOLDER_PKG">
<description>1xAAA battery holder, eagle plastics 12bH411P-R-GR</description>
</package>
<package name="P398DLP_RADIOFEATHER_M0_PKG">
<description>Adafruit RadioFeather M0</description>
</package>
<package name="P398DLP_74HC137N_PKG">
<description>CD74HC137 1-of-8 demux</description>
</package>
<package name="P398DLP_TTL_SERIAL_CAMERA_PKG">
<description>VC0706 TTL Serial Camera</description>
</package>
<package name="P398DLP_ROSEGRAPHIC_PKG">
<description>VL53L0X proximity sensor</description>
</package>
<package name="P398DLP_PUSHBUTTON_PKG">
<description>pushbutton</description>
</package>
<package name="P398DLP_SPDT_SWITCH_PKG">
<description>pushbutton</description>
</package>
<package name="P398DLP_GAS_SENSOR_PKG">
<description>&lt;h3&gt;Gas Sensors - MQ-3, MQ-4, MQ-6, MQ-7, MQ-8&lt;/h3&gt;
&lt;p&gt;Footprint is orientation agnostic: A and B pins can be exchanged.&lt;/p&gt;
&lt;p&gt;&lt;a href="https://cdn.sparkfun.com/datasheets/Sensors/Biometric/MQ-3%20ver1.3%20-%20Manual.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;
&lt;li&gt;Pin Count: 6&lt;/li&gt;
&lt;li&gt;Diameter: 14.5 mm&lt;/li&gt;
&lt;/ul&gt;
&lt;p&gt;Devices Using:&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;GAS_SENSOR&lt;/li&gt;
&lt;/ul&gt;</description>
</package>
<package name="SOT-25">
</package>
<package name="P398DLP_AP2112_PKG">
<description>AP2112: LDO 3.3 V regulator</description>
</package>
<package name="DIL18">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="SOCKET-18">
<description>&lt;b&gt;Dual In Line Socket&lt;/b&gt;</description>
</package>
<package name="P398DLP_MCP23008_PKG">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="P398DLP_1N5817_PKG">
<description>1N5817 Schottky barrier diode</description>
</package>
<package name="DO41-7.6">
<description>&lt;b&gt;DO41&lt;/b&gt; 7.6mm x 2mm&lt;p&gt;
Source: http://www.diodes.com/datasheets/ds23001.pdf</description>
</package>
<package name="P398DLP_TPS7133Q_PKG">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="P398DLP_AIRLIFT_PKG">
<description>Adafruit AirLift WiFi module</description>
</package>
<package name="P398DLP_TSOP38238_PKG">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="P398DLP_MOUNTING_HOLE_PKG">
<description>0.1 inch diameter (mounting) hole</description>
</package>
<package name="P398DLP_MOLEX_DUAL_USB-A_PKG">
<description>molex dual USB-A connector, female</description>
</package>
<package name="USB">
<description>&lt;b&gt;USB connector&lt;/b&gt;</description>
</package>
<package name="P398DLP_FRAM_PKG">
<description>32kB FRAM I2C memory</description>
</package>
<package name="P398DLP_ADG436_SWITCH_PKG">
<description>Analog Devices ADG436 dual SPDT analog switch</description>
</package>
<package name="P398DLP_JUMPER_PKG">
</package>
<package name="P398DLP_SLIDE_SWITCH_PKG">
<description>slide switch, 0.3" through hole digikey KG01ET</description>
</package>
<package name="P398DLP_FEATHER_M4_EXPRESS_PKG">
<description>uit Feather M4 Express with samd51 processor</description>
</package>
<package name="P398DLP_MOLEX_USB-A_PKG">
<description>molex female USB-A 67643-3910</description>
</package>
<package name="P398DLP_USB-A_MICRO_USB_CABLE">
</package>
<package name="P398DLP_USB-A_MICRO_USB_CABLE_HOLLOW_PKG">
</package>
<package name="P398DLP_RESISTOR_SIP7_PKG">
<description>Bourns 4607X-101 SIP 6 resistor array</description>
</package>
<package name="P398DLP_MOUNTING_HOLE_4MM_PKG">
</package>
<package name="P398DLP_ARDUINO_MEGA2560_PKG">
<description>Arduino MEGA 2560, component side DOWN</description>
</package>
<package name="P398DLP_SPST_SWITCH_PKG">
</package>
<package name="P398DLP_LORA_BREAKOUT_PKG">
<description>LoRa 915 MHz breakout, Adafruit 3072</description>
</package>
<package name="P398DLP_SPDT_SWITCH_2MM_PKG">
<description>SPDT slide switch, 2mm pitch: CKSwitches.com, OS102011MS2QN1</description>
</package>
<package name="P398DLP_BLUETOOTH_FRIEND_PKG">
<description>Adafruit Bluetooth LE SPI friend: 2633</description>
</package>
<package name="P398DLP_MICS5524_CO_PKG">
<description>MiCS5524 CO, Alcohol, and VOC gas sensor
Adafruit 3199</description>
</package>
<package name="P398DLP_PULSE_SENSOR_PKG">
<description>WorldFamousElectronics pulse sensor</description>
</package>
<package name="P398DLP_BME680_STEMMA_PKG">
<description>BME680 T/P/RH/VOC STEMMA connector</description>
</package>
<package name="P398DLP_2XAA_BATTERY_PKG">
<description>2xAA battery pack</description>
</package>
<package name="P398DLP_SPDT_DIP_SLIDE_SWITCH_PKG">
<description>SPDT slide switch, .098 inch pitch: EG1218 E-SWITCH, Adafruit 805</description>
</package>
<package name="P398DLP_MOUNTING_HOLE_300MIL_PKG">
<description>0.3 inch diameter hole</description>
</package>
<package name="P398DLP_BQ24074_SOLAR_CHARGER_PKG">
<description>Adafruit bq24074 solar power charger: part ID 4755</description>
</package>
<package name="P398DLP_USB_MICRO_BREAKOUT_PKG">
<description>Adafruit 1833 microUSB breakout</description>
</package>
<package name="P398DLP_MOUNTING_HOLE_250MIL_PKG">
<description>0.25 inch diameter hole</description>
</package>
<package name="P398DLP_USB_C_BREAKOUT_PKG">
<description>Adafruit 4090 USB-C breakout</description>
</package>
<package name="P398DLP_VOLTMETER_PKG">
<description>Adafruit 2-wire voltmeter</description>
</package>
<package name="P398DLP_ADC_QUAD_I2C_PKG">
<description>Adafruit ADS1015 quad ADC</description>
</package>
<package name="P398DLP_DPS310_PKG">
<description>DPS310 precision pressure and temperature sensor. Adafruit 4494</description>
</package>
<package name="06V">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;</description>
</package>
<package name="P398DLP_MCP4728_PKG">
<description>MCP4728 quad 12-bit DAC Adafruit 4470</description>
</package>
<package name="P398DLP_AS7262_PKG">
<description>MCP4728 quad 12-bit DAC Adafriuit 4470</description>
</package>
<package name="P398DLP_NPN_PKG">
<description>NPN transistor, TO-92 case</description>
</package>
<package name="P398DLP_SONY_SPRESENSE_EXTENSION_PKG">
<description>Sony Spresense extension board</description>
</package>
<package name="P398DLP_MLX90640_CAMERA_PKG">
<description>MLX90640 low resolution IR camera. Adafruit 4407</description>
</package>
<package name="P398DLP_RED_LED_PKG">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="P398DLP_ROTARY_SWITCH_PKG">
<description>CTSCORP.com rotary switch
220ADC16</description>
</package>
<package name="P398DLP_ROSE4_PKG">
<description>rose bitmap</description>
</package>
<package name="P398DLP_TFT_DISPLAY_PKG">
<description>160x128 TFT display</description>
</package>
<package name="P398DLP_LC709203F_STEMMA_PKG">
<description>LC709203F LiPo "fuel gauge"</description>
</package>
<package name="P398DLP_PUSHBUTTON2A_PKG">
<description>Pushbutton</description>
</package>
<package name="P398DLP_AS7341_PKG">
<description>AS7341 10 channel spectrometer</description>
</package>
<package name="P398DLP_PHOTO_INTERRUPTER_PKG">
<description>Adafruit four-wire photo interrupter</description>
</package>
<package name="P398DLP_SFM3300_HEADER_PKG">
<description>Sensirion SFM3300 flowmeter header</description>
</package>
<package name="P398DLP_DC_DC_CONVERTER_PKG">
<description>RECOM ROE SIP4 DC-DC converter
3,3 V to 5 V
ROE-3..305S part number</description>
</package>
<package name="P398DLP_L4931_REG_PKG">
<description>L4931 linear voltage regulator, TO-92 case
5.0V, adafruit 2236</description>
</package>
<package name="P398DLP_MAX30102_SPARKFUN_PKG">
<description>SparkFun Max30102 board
P398DLP_MAX30102_SPARKFUN</description>
</package>
<package name="P398DLP_ADXL375_PKG">
<description>ADXL375 200 g accelerometer</description>
</package>
<package name="P398DLP_H3LIS331_PKG">
<description>H3LIS331 400 g accelerometer</description>
</package>
</packages>
<symbols>
<symbol name="P398DLP_ADXL326_SYM">
<description>ADXL326 3 axis accelerometer</description>
<pin name="VIN"/>
<pin name="3VO"/>
<pin name="GND"/>
<pin name="ZOUT"/>
<pin name="YOUT"/>
<pin name="XOUT"/>
<pin name="TEST"/>
</symbol>
<symbol name="P398DLP_BME680_SYM">
<description>BME680 temperature, pressure, relative humidity, and volatile organic compounds sensor</description>
<pin name="VIN"/>
<pin name="3V0"/>
<pin name="GND"/>
<pin name="SCK"/>
<pin name="SDO"/>
<pin name="SDI"/>
<pin name="CS"/>
</symbol>
<symbol name="P398DLP_MICROSD_SYM">
<description>Adafruit microSD reader breakout board</description>
<pin name="5V"/>
<pin name="3V"/>
<pin name="GND"/>
<pin name="CLK"/>
<pin name="DO"/>
<pin name="DI"/>
<pin name="CS"/>
<pin name="CD"/>
</symbol>
<symbol name="P398DLP_MCP4725_SYM">
<description>MCP4725 12-bit DAC</description>
<pin name="VDD"/>
<pin name="GND"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="A0"/>
<pin name="VOUT"/>
</symbol>
<symbol name="P398DLP_DS3231_SYM">
<description>DS3231 real time clock with battery backup</description>
<pin name="VIN"/>
<pin name="GND"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="BAT"/>
<pin name="32K"/>
<pin name="SQW"/>
<pin name="RSTBAR"/>
</symbol>
<symbol name="PINHD7">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
</symbol>
<symbol name="PINHD3">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
</symbol>
<symbol name="PINHD4">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
</symbol>
<symbol name="PINHD5">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
</symbol>
<symbol name="PINHD6">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
</symbol>
<symbol name="PINHD8">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
</symbol>
<symbol name="PINHD9">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
</symbol>
<symbol name="PINHD10">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
</symbol>
<symbol name="PINHD11">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
</symbol>
<symbol name="PINHD12">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
<pin name="12" direction="pas" function="dot"/>
</symbol>
<symbol name="PINH2X18">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
<pin name="12" direction="pas" function="dot"/>
<pin name="13" direction="pas" function="dot"/>
<pin name="14" direction="pas" function="dot"/>
<pin name="15" direction="pas" function="dot"/>
<pin name="16" direction="pas" function="dot"/>
<pin name="17" direction="pas" function="dot"/>
<pin name="18" direction="pas" function="dot"/>
<pin name="19" direction="pas" function="dot"/>
<pin name="20" direction="pas" function="dot"/>
<pin name="21" direction="pas" function="dot"/>
<pin name="22" direction="pas" function="dot"/>
<pin name="23" direction="pas" function="dot"/>
<pin name="24" direction="pas" function="dot"/>
<pin name="25" direction="pas" function="dot"/>
<pin name="26" direction="pas" function="dot"/>
<pin name="27" direction="pas" function="dot"/>
<pin name="28" direction="pas" function="dot"/>
<pin name="29" direction="pas" function="dot"/>
<pin name="30" direction="pas" function="dot"/>
<pin name="31" direction="pas" function="dot"/>
<pin name="32" direction="pas" function="dot"/>
<pin name="33" direction="pas" function="dot"/>
<pin name="34" direction="pas" function="dot"/>
<pin name="35" direction="pas" function="dot"/>
<pin name="36" direction="pas" function="dot"/>
</symbol>
<symbol name="AMP_GND_GAIN_BYP">
<pin name="GAIN@1" direction="pas"/>
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="GAIN@2" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="5V" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="BYPASS" direction="pas"/>
</symbol>
<symbol name="PINHD16">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
<pin name="12" direction="pas" function="dot"/>
<pin name="13" direction="pas" function="dot"/>
<pin name="14" direction="pas" function="dot"/>
<pin name="15" direction="pas" function="dot"/>
<pin name="16" direction="pas" function="dot"/>
</symbol>
<symbol name="POT_US-">
<pin name="A" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="S" direction="pas"/>
</symbol>
<symbol name="MEGA_SYMBOL">
<description>Symbol as Mega card</description>
<pin name="AREF"/>
<pin name="GND@1"/>
<pin name="13"/>
<pin name="12"/>
<pin name="11"/>
<pin name="10"/>
<pin name="9"/>
<pin name="8"/>
<pin name="7"/>
<pin name="6"/>
<pin name="5"/>
<pin name="4"/>
<pin name="3"/>
<pin name="2"/>
<pin name="1"/>
<pin name="0"/>
<pin name="14"/>
<pin name="15"/>
<pin name="16"/>
<pin name="17"/>
<pin name="18"/>
<pin name="19"/>
<pin name="20"/>
<pin name="21"/>
<pin name="GND@4"/>
<pin name="GND@5"/>
<pin name="23"/>
<pin name="25"/>
<pin name="27"/>
<pin name="29"/>
<pin name="31"/>
<pin name="33"/>
<pin name="35"/>
<pin name="37"/>
<pin name="39"/>
<pin name="41"/>
<pin name="43"/>
<pin name="45"/>
<pin name="47"/>
<pin name="49"/>
<pin name="51"/>
<pin name="53"/>
<pin name="GND@7"/>
<pin name="22"/>
<pin name="24"/>
<pin name="26"/>
<pin name="28"/>
<pin name="30"/>
<pin name="32"/>
<pin name="34"/>
<pin name="36"/>
<pin name="38"/>
<pin name="40"/>
<pin name="42"/>
<pin name="44"/>
<pin name="46"/>
<pin name="48"/>
<pin name="50"/>
<pin name="52"/>
<pin name="GND@6"/>
<pin name="A15"/>
<pin name="A14"/>
<pin name="A13"/>
<pin name="A12"/>
<pin name="A11"/>
<pin name="A10"/>
<pin name="A9"/>
<pin name="A8"/>
<pin name="A7"/>
<pin name="A6"/>
<pin name="A5"/>
<pin name="A4"/>
<pin name="A3"/>
<pin name="A2"/>
<pin name="A1"/>
<pin name="A0"/>
<pin name="VIN"/>
<pin name="GND@3"/>
<pin name="GND@2"/>
<pin name="5V"/>
<pin name="3V3"/>
<pin name="RESET"/>
</symbol>
<symbol name="P398DLP_MICROPHONE_SYM">
<description>Adafruit amplified electret microphone</description>
<pin name="OUT" direction="pas" function="dot"/>
<pin name="GND" direction="pas" function="dot"/>
<pin name="VCC" direction="pas" function="dot"/>
</symbol>
<symbol name="P398DLP_ULTIMATE_GPS_SYM">
<description>Adafruit "ultimate GPS" breakout board</description>
<pin name="3.3V" direction="pas" function="dot"/>
<pin name="EN" direction="pas" function="dot"/>
<pin name="VBAT" direction="pas" function="dot"/>
<pin name="FIX" direction="pas" function="dot"/>
<pin name="TX" direction="pas" function="dot"/>
<pin name="RX" direction="pas" function="dot"/>
<pin name="GND" direction="pas" function="dot"/>
<pin name="VIN" direction="pas" function="dot"/>
<pin name="PPS" direction="pas" function="dot"/>
</symbol>
<symbol name="P398DLP_SPEAKER_SYM">
<description>0.5 watt, 8 ohm mini-metal speaker</description>
<pin name="VIN+" direction="pas" function="dot"/>
<pin name="VIN-" direction="pas" function="dot"/>
</symbol>
<symbol name="PINHD2">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
</symbol>
<symbol name="P398DLP_PUSHBUTTON_SYM">
<description>pushbutton</description>
<pin name="PIN1" direction="pas" function="dot"/>
<pin name="NC" direction="pas" function="dot"/>
<pin name="PIN2" direction="pas" function="dot"/>
</symbol>
<symbol name="P398DLP_INA219_SYM">
<description>INA219 current/voltage sensor</description>
<pin name="VCC" direction="pas" function="dot"/>
<pin name="GND" direction="pas" function="dot"/>
<pin name="SCL" direction="pas" function="dot"/>
<pin name="SDA" direction="pas" function="dot"/>
<pin name="VIN-" direction="pas" function="dot"/>
<pin name="VIN+" direction="pas" function="dot"/>
</symbol>
<symbol name="MLX90614">
<description>&lt;h3&gt;Melexis MLX90614 Infrared (IR) Thermometer&lt;/h3&gt;
&lt;p&gt;The MLX90614 is a passive infrared (PIR) I&lt;sup&gt;2&lt;/sup&gt;C temperature sensor.It is designed for non-contact temperature sensing. An internal 17-bit ADC and a powerful DSP contribute to the MLX90614’s high accuracy and resolution. It has a huge number of applications including body temperature measurment and movement detection.&lt;/p&gt;</description>
<pin name="VDD"/>
<pin name="VSS"/>
<pin name="SCL/VZ"/>
<pin name="PWM/SDA"/>
</symbol>
<symbol name="P398DLP_LCD_16X2_SYM">
<description>2x16 liquid crystal display, four mounting holes.
Crystalfontz CFAH1602B-NGG-JTV</description>
<pin name="PULL" direction="out"/>
<pin name="DB0"/>
<pin name="DB1"/>
<pin name="DB2"/>
<pin name="DB3"/>
<pin name="DB4"/>
<pin name="DB5"/>
<pin name="DB6"/>
<pin name="DB7"/>
<pin name="E" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="R/W" direction="in"/>
<pin name="RS" direction="in"/>
<pin name="5V"/>
<pin name="VO"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="P398DLP_KEYPAD_SYM">
<description>3x4 telephone-style keypad</description>
<pin name="COL1" direction="pas" function="dot"/>
<pin name="COL2" direction="pas" function="dot"/>
<pin name="COL3" direction="pas" function="dot"/>
<pin name="ROW1" direction="pas" function="dot"/>
<pin name="ROW2" direction="pas" function="dot"/>
<pin name="ROW3" direction="pas" function="dot"/>
<pin name="ROW4" direction="pas" function="dot"/>
<pin name="NC" direction="pas" function="dot"/>
</symbol>
<symbol name="P398DLP_5XAA_BATTERY_SYM">
<description>5xAA battery holder</description>
<pin name="BATTERY_7.5V" direction="pas" function="dot"/>
<pin name="BATTERY_GND" direction="pas" function="dot"/>
</symbol>
<symbol name="PINHD2-1">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
</symbol>
<symbol name="PINHD1">
<pin name="1" direction="pas" function="dot"/>
</symbol>
<symbol name="P398DLP_PAM8302A_SYM">
<description>PAM8302A PWM audio amplifier</description>
<pin name="A+" direction="in"/>
<pin name="A-" direction="in"/>
<pin name="SD_BAR" direction="in"/>
<pin name="VIN"/>
<pin name="GND"/>
<pin name="VO+" direction="out"/>
<pin name="VO-" direction="out"/>
</symbol>
<symbol name="P398DLP_TSL2561_SYM">
<description>TSL2561 Lux Sensor</description>
<pin name="VIN"/>
<pin name="GND"/>
<pin name="3.3V"/>
<pin name="ADDR"/>
<pin name="INT"/>
<pin name="SDA_5V"/>
<pin name="SCL_5V"/>
</symbol>
<symbol name="P398DLP_GUVA_ANALOG_UV_SYM">
<description>GUVA UV sensor</description>
<pin name="GND"/>
<pin name="AOUT" direction="out"/>
<pin name="5.0V"/>
</symbol>
<symbol name="P398DLP_ARDUINO_FLIPPED_SYM">
<description>Arduino MEGA 2560, components down</description>
<pin name="SCL1" direction="pas" function="dot"/>
<pin name="SDA1" direction="pas" function="dot"/>
<pin name="AREF" direction="pas" function="dot"/>
<pin name="GND3" direction="pas" function="dot"/>
<pin name="D13" direction="pas" function="dot"/>
<pin name="D12" direction="pas" function="dot"/>
<pin name="D11" direction="pas" function="dot"/>
<pin name="D10" direction="pas" function="dot"/>
<pin name="D9" direction="pas" function="dot"/>
<pin name="D8" direction="pas" function="dot"/>
<pin name="D7" direction="pas" function="dot"/>
<pin name="D6" direction="pas" function="dot"/>
<pin name="D5" direction="pas" function="dot"/>
<pin name="D4" direction="pas" function="dot"/>
<pin name="D3" direction="pas" function="dot"/>
<pin name="D2" direction="pas" function="dot"/>
<pin name="D1&lt;-TX" direction="pas" function="dot"/>
<pin name="D0-&gt;RX" direction="pas" function="dot"/>
<pin name="D14TX3" direction="pas" function="dot"/>
<pin name="D15RX3" direction="pas" function="dot"/>
<pin name="D16TX2" direction="pas" function="dot"/>
<pin name="D17RX2" direction="pas" function="dot"/>
<pin name="D18TX1" direction="pas" function="dot"/>
<pin name="D19RX1" direction="pas" function="dot"/>
<pin name="D20SDA" direction="pas" function="dot"/>
<pin name="D21SCL" direction="pas" function="dot"/>
<pin name="NC" direction="pas" function="dot"/>
<pin name="IOREF" direction="pas" function="dot"/>
<pin name="RESET" direction="pas" function="dot"/>
<pin name="3.3V" direction="pas" function="dot"/>
<pin name="5V1" direction="pas" function="dot"/>
<pin name="GND1" direction="pas" function="dot"/>
<pin name="GND2" direction="pas" function="dot"/>
<pin name="VIN" direction="pas" function="dot"/>
<pin name="A0" direction="pas" function="dot"/>
<pin name="A1" direction="pas" function="dot"/>
<pin name="A2" direction="pas" function="dot"/>
<pin name="A3" direction="pas" function="dot"/>
<pin name="A4" direction="pas" function="dot"/>
<pin name="A5" direction="pas" function="dot"/>
<pin name="A6" direction="pas" function="dot"/>
<pin name="A7" direction="pas" function="dot"/>
<pin name="A8" direction="pas" function="dot"/>
<pin name="A9" direction="pas" function="dot"/>
<pin name="A10" direction="pas" function="dot"/>
<pin name="A11" direction="pas" function="dot"/>
<pin name="A12" direction="pas" function="dot"/>
<pin name="A13" direction="pas" function="dot"/>
<pin name="A14" direction="pas" function="dot"/>
<pin name="A15" direction="pas" function="dot"/>
<pin name="GND4" direction="pas" function="dot"/>
<pin name="GND5" direction="pas" function="dot"/>
<pin name="D52" direction="pas" function="dot"/>
<pin name="D53" direction="pas" function="dot"/>
<pin name="D50" direction="pas" function="dot"/>
<pin name="D51" direction="pas" function="dot"/>
<pin name="D48" direction="pas" function="dot"/>
<pin name="D49" direction="pas" function="dot"/>
<pin name="D46" direction="pas" function="dot"/>
<pin name="D47" direction="pas" function="dot"/>
<pin name="D44" direction="pas" function="dot"/>
<pin name="D45" direction="pas" function="dot"/>
<pin name="D42" direction="pas" function="dot"/>
<pin name="D43" direction="pas" function="dot"/>
<pin name="D40" direction="pas" function="dot"/>
<pin name="D41" direction="pas" function="dot"/>
<pin name="D38" direction="pas" function="dot"/>
<pin name="D39" direction="pas" function="dot"/>
<pin name="D36" direction="pas" function="dot"/>
<pin name="D37" direction="pas" function="dot"/>
<pin name="D34" direction="pas" function="dot"/>
<pin name="D35" direction="pas" function="dot"/>
<pin name="D32" direction="pas" function="dot"/>
<pin name="D33" direction="pas" function="dot"/>
<pin name="D30" direction="pas" function="dot"/>
<pin name="D31" direction="pas" function="dot"/>
<pin name="D28" direction="pas" function="dot"/>
<pin name="D29" direction="pas" function="dot"/>
<pin name="D26" direction="pas" function="dot"/>
<pin name="D27" direction="pas" function="dot"/>
<pin name="D24" direction="pas" function="dot"/>
<pin name="D25" direction="pas" function="dot"/>
<pin name="D22" direction="pas" function="dot"/>
<pin name="D23" direction="pas" function="dot"/>
<pin name="5V2" direction="pas" function="dot"/>
<pin name="5V3" direction="pas" function="dot"/>
<pin name="BATTERY_7.5V" direction="pas" function="dot"/>
<pin name="BATTERY_GND" direction="pas" function="dot"/>
<pin name="_D48" direction="pas" function="dot"/>
<pin name="_D46" direction="pas" function="dot"/>
<pin name="_D44" direction="pas" function="dot"/>
<pin name="_D42" direction="pas" function="dot"/>
<pin name="_D40" direction="pas" function="dot"/>
<pin name="_D38" direction="pas" function="dot"/>
<pin name="_D36" direction="pas" function="dot"/>
<pin name="_D34" direction="pas" function="dot"/>
<pin name="_D32" direction="pas" function="dot"/>
<pin name="_D30" direction="pas" function="dot"/>
<pin name="_D28" direction="pas" function="dot"/>
<pin name="_D26" direction="pas" function="dot"/>
<pin name="_D24" direction="pas" function="dot"/>
<pin name="_D53" direction="pas" function="dot"/>
<pin name="_D51" direction="pas" function="dot"/>
<pin name="_D49" direction="pas" function="dot"/>
<pin name="_D47" direction="pas" function="dot"/>
<pin name="_D45" direction="pas" function="dot"/>
<pin name="_D43" direction="pas" function="dot"/>
<pin name="_D41" direction="pas" function="dot"/>
<pin name="_D39" direction="pas" function="dot"/>
<pin name="_D37" direction="pas" function="dot"/>
<pin name="_D35" direction="pas" function="dot"/>
<pin name="_D33" direction="pas" function="dot"/>
<pin name="_D31" direction="pas" function="dot"/>
<pin name="_D29" direction="pas" function="dot"/>
<pin name="_D27" direction="pas" function="dot"/>
<pin name="_D25" direction="pas" function="dot"/>
<pin name="_D23" direction="pas" function="dot"/>
<pin name="_D14TX3" direction="pas" function="dot"/>
<pin name="_D15RX3" direction="pas" function="dot"/>
<pin name="_D16TX2" direction="pas" function="dot"/>
<pin name="_D17RX2" direction="pas" function="dot"/>
<pin name="_D18TX1" direction="pas" function="dot"/>
<pin name="_D19RX1" direction="pas" function="dot"/>
<pin name="_D20SDA" direction="pas" function="dot"/>
<pin name="_D21SCL" direction="pas" function="dot"/>
<pin name="_D7" direction="pas" function="dot"/>
<pin name="_D6" direction="pas" function="dot"/>
<pin name="_D5" direction="pas" function="dot"/>
<pin name="_D4" direction="pas" function="dot"/>
<pin name="_D3" direction="pas" function="dot"/>
<pin name="_D2" direction="pas" function="dot"/>
<pin name="_D1&lt;-TX" direction="pas" function="dot"/>
<pin name="_D0-&gt;RX" direction="pas" function="dot"/>
<pin name="_A8" direction="pas" function="dot"/>
<pin name="_A9" direction="pas" function="dot"/>
<pin name="_A10" direction="pas" function="dot"/>
<pin name="_A11" direction="pas" function="dot"/>
<pin name="_A12" direction="pas" function="dot"/>
<pin name="_A13" direction="pas" function="dot"/>
<pin name="_A14" direction="pas" function="dot"/>
<pin name="_A15" direction="pas" function="dot"/>
<pin name="_A0" direction="pas" function="dot"/>
<pin name="_A1" direction="pas" function="dot"/>
<pin name="_A2" direction="pas" function="dot"/>
<pin name="_A3" direction="pas" function="dot"/>
<pin name="_A4" direction="pas" function="dot"/>
<pin name="_A5" direction="pas" function="dot"/>
<pin name="_A6" direction="pas" function="dot"/>
<pin name="_A7" direction="pas" function="dot"/>
<pin name="_IOREF" direction="pas" function="dot"/>
<pin name="_RESET" direction="pas" function="dot"/>
<pin name="_VIN" direction="pas" function="dot"/>
<pin name="_SCL1" direction="pas" function="dot"/>
<pin name="_SDA1" direction="pas" function="dot"/>
<pin name="_AREF" direction="pas" function="dot"/>
<pin name="_D13" direction="pas" function="dot"/>
<pin name="_D12" direction="pas" function="dot"/>
<pin name="_D11" direction="pas" function="dot"/>
<pin name="_D10" direction="pas" function="dot"/>
<pin name="_D9" direction="pas" function="dot"/>
<pin name="_D8" direction="pas" function="dot"/>
</symbol>
<symbol name="P398DLP_VL53L0X_SYM">
<description>VL53L0X proximity sensor</description>
<pin name="VIN" direction="pas" function="dot"/>
<pin name="2V8" direction="pas" function="dot"/>
<pin name="GND" direction="pas" function="dot"/>
<pin name="GPIO" direction="pas" function="dot"/>
<pin name="SHDN" direction="pas" function="dot"/>
<pin name="SCL" direction="pas" function="dot"/>
<pin name="SDA" direction="pas" function="dot"/>
</symbol>
<symbol name="P398DLP_L3GD20H_SYM">
<description>L3GD20H 3-axis gyro</description>
<pin name="SCL" direction="pas" function="dot"/>
<pin name="SDA" direction="pas" function="dot"/>
<pin name="SA0" direction="pas" function="dot"/>
<pin name="CS" direction="pas" function="dot"/>
<pin name="DRDY" direction="pas" function="dot"/>
<pin name="INT1" direction="pas" function="dot"/>
<pin name="GND" direction="pas" function="dot"/>
<pin name="3VOUT" direction="pas" function="dot"/>
<pin name="VCC" direction="pas" function="dot"/>
</symbol>
<symbol name="P398DLP_ON-OFF-ON-OFF_SWITCH_SYM">
<description>on-off-on-off pushbutton switch</description>
<pin name="LEFT" direction="pas" function="dot"/>
<pin name="CENTER" direction="pas" function="dot"/>
<pin name="RIGHT" direction="pas" function="dot"/>
</symbol>
<symbol name="P398DLP_TRIMPOT_SYM">
<description>trimpot</description>
<pin name="BOTTOM" direction="pas"/>
<pin name="TOP" direction="pas"/>
<pin name="TAP" direction="pas"/>
</symbol>
<symbol name="P398DLP_MLX90614_IR_SYM">
<description>&lt;h3&gt;Melexis MLX90614 Infrared (IR) Thermometer&lt;/h3&gt;
&lt;p&gt;The MLX90614 is a passive infrared (PIR) I&lt;sup&gt;2&lt;/sup&gt;C temperature sensor.It is designed for non-contact temperature sensing. An internal 17-bit ADC and a powerful DSP contribute to the MLX90614’s high accuracy and resolution. It has a huge number of applications including body temperature measurment and movement detection.&lt;/p&gt;</description>
<pin name="VDD"/>
<pin name="VSS"/>
<pin name="SCL/VZ"/>
<pin name="PWM/SDA"/>
</symbol>
<symbol name="P398DLP_LSM9DS1_9DOF_SYM">
<description>LSM9DS1 accelerometer, gyroscope, magnetometer</description>
<pin name="VIN" direction="pas" function="dot"/>
<pin name="3V3" direction="pas" function="dot"/>
<pin name="GND" direction="pas" function="dot"/>
<pin name="SCL" direction="pas" function="dot"/>
<pin name="SDA" direction="pas" function="dot"/>
<pin name="CSAG" direction="pas" function="dot"/>
<pin name="CSM" direction="pas" function="dot"/>
<pin name="SDOAG" direction="pas" function="dot"/>
<pin name="SDOM" direction="pas" function="dot"/>
<pin name="DEN" direction="pas" function="dot"/>
<pin name="INT2" direction="pas" function="dot"/>
<pin name="INT1" direction="pas" function="dot"/>
<pin name="DRDY" direction="pas" function="dot"/>
<pin name="INTM" direction="pas" function="dot"/>
</symbol>
<symbol name="P398DLP_MMA8451_ACCEL_SYM">
<description>MMA8451 3-axis accelerometer</description>
<pin name="VIN"/>
<pin name="GND"/>
<pin name="3VO"/>
<pin name="I2"/>
<pin name="I1"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="A"/>
</symbol>
<symbol name="P398DLP_FORCE_SENSITIVE_RESISTOR_SYM">
<pin name="FSR2" direction="pas"/>
<pin name="5V/FSR1" direction="pas"/>
</symbol>
<symbol name="R-US">
<pin name="FSR2" direction="pas"/>
<pin name="5V/FSR1" direction="pas"/>
</symbol>
<symbol name="P398DLP_ANEMOMETER_SYM">
<pin name="GND" direction="pas"/>
<pin name="7.5V" direction="pas"/>
<pin name="ANEMOMETER" direction="pas"/>
</symbol>
<symbol name="P398DLP_MYOWARE_SYM">
<description>myoware EMG sensor</description>
<pin name="GND" direction="pas"/>
<pin name="5V" direction="pas"/>
<pin name="MYOWARE" direction="pas"/>
</symbol>
<symbol name="P398DLP_GP2Y0A21YK0F_IR_PROXIMITY_SYM">
<description>IR proximity sensor</description>
<pin name="GND" direction="pas"/>
<pin name="5V" direction="pas"/>
<pin name="IR_PROXIMITY" direction="pas"/>
</symbol>
<symbol name="P398DLP_POWER+ADC_SYM">
<description>ADC + power + ground</description>
<pin name="GND" direction="pas"/>
<pin name="5V" direction="pas"/>
<pin name="ADC" direction="pas"/>
</symbol>
<symbol name="P398DLP_PMS5003_PM2.5_SYM">
<description>PMS5003 airborne particulates sensor</description>
<pin name="VCC" direction="pas" function="dot"/>
<pin name="GND" direction="pas" function="dot"/>
<pin name="SET" direction="pas" function="dot"/>
<pin name="RXD" direction="pas" function="dot"/>
<pin name="TXD" direction="pas" function="dot"/>
<pin name="RST" direction="pas" function="dot"/>
<pin name="NC1" direction="pas" function="dot"/>
<pin name="NC2" direction="pas" function="dot"/>
</symbol>
<symbol name="P398DLP_TCA9548A_MUX_SYM">
<description>TCA9548A I2C MUX</description>
<pin name="VIN" direction="pas" function="dot"/>
<pin name="GND" direction="pas" function="dot"/>
<pin name="SDA" direction="pas" function="dot"/>
<pin name="SCL" direction="pas" function="dot"/>
<pin name="RST" direction="pas" function="dot"/>
<pin name="A0" direction="pas" function="dot"/>
<pin name="A1" direction="pas" function="dot"/>
<pin name="A2" direction="pas" function="dot"/>
<pin name="SD0" direction="pas" function="dot"/>
<pin name="SC6" direction="pas" function="dot"/>
<pin name="SD6" direction="pas" function="dot"/>
<pin name="SC5" direction="pas" function="dot"/>
<pin name="SD5" direction="pas" function="dot"/>
<pin name="SC4" direction="pas" function="dot"/>
<pin name="SC0" direction="pas" function="dot"/>
<pin name="SD1" direction="pas" function="dot"/>
<pin name="SC1" direction="pas" function="dot"/>
<pin name="SC7" direction="pas" function="dot"/>
<pin name="SD7" direction="pas" function="dot"/>
<pin name="SD4" direction="pas" function="dot"/>
<pin name="SC3" direction="pas" function="dot"/>
<pin name="SD3" direction="pas" function="dot"/>
<pin name="SC2" direction="pas" function="dot"/>
<pin name="SD2" direction="pas" function="dot"/>
</symbol>
<symbol name="P398DLP_DRV2605L_HAPTIC_SYM">
<description>DRV2605L haptic (vibrator) driver</description>
<pin name="VIN" direction="pas" function="dot"/>
<pin name="GND" direction="pas" function="dot"/>
<pin name="SCL" direction="pas" function="dot"/>
<pin name="SDA" direction="pas" function="dot"/>
<pin name="IN" direction="pas" function="dot"/>
<pin name="MOTOR+" direction="pas" function="dot"/>
<pin name="MOTOR-" direction="pas" function="dot"/>
</symbol>
<symbol name="P398DLP_HAPTIC_VIBRATOR_MOTOR_SYM">
<description>haptic vibrator</description>
<pin name="MOTOR-" direction="pas"/>
<pin name="MOTOR+" direction="pas"/>
</symbol>
<symbol name="P398DLP_POWER+I2C_SYM">
<description>powered I2C connection</description>
<pin name="GND" direction="pas"/>
<pin name="5V" direction="pas"/>
<pin name="SDA" direction="pas"/>
<pin name="SCL" direction="pas"/>
</symbol>
<symbol name="P398DLP_ADALOGGER_M0_SYM">
<description>Adafruit Adalogger M0 processor</description>
<pin name="RST"/>
<pin name="3V"/>
<pin name="AREF"/>
<pin name="GND"/>
<pin name="A0"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="SCK"/>
<pin name="MOSI"/>
<pin name="MISO"/>
<pin name="RX"/>
<pin name="TX"/>
<pin name="GND2"/>
<pin name="SDA"/>
<pin name="SCL"/>
<pin name="#5"/>
<pin name="#6"/>
<pin name="#9"/>
<pin name="#10"/>
<pin name="#11"/>
<pin name="#12"/>
<pin name="#13"/>
<pin name="USB"/>
<pin name="EN"/>
<pin name="BAT"/>
</symbol>
<symbol name="P398DLP_74HC157N_SYM">
<pin name="!A!/B" direction="in"/>
<pin name="1A" direction="in"/>
<pin name="1B" direction="in"/>
<pin name="1Y" direction="out"/>
<pin name="2A" direction="in"/>
<pin name="2B" direction="in"/>
<pin name="2Y" direction="out"/>
<pin name="3Y" direction="out"/>
<pin name="3B" direction="in"/>
<pin name="3A" direction="in"/>
<pin name="4Y" direction="out"/>
<pin name="4B" direction="in"/>
<pin name="4A" direction="in"/>
<pin name="G" direction="in" function="dot"/>
<pin name="GND"/>
<pin name="VCC"/>
</symbol>
<symbol name="74157">
<description>SN74HC157N is a PDIP quad 2:1 multiplexer.</description>
<pin name="!A!/B" direction="in"/>
<pin name="1A" direction="in"/>
<pin name="1B" direction="in"/>
<pin name="1Y" direction="out"/>
<pin name="2A" direction="in"/>
<pin name="2B" direction="in"/>
<pin name="2Y" direction="out"/>
<pin name="3Y" direction="out"/>
<pin name="3B" direction="in"/>
<pin name="3A" direction="in"/>
<pin name="4Y" direction="out"/>
<pin name="4B" direction="in"/>
<pin name="4A" direction="in"/>
<pin name="G" direction="in" function="dot"/>
</symbol>
<symbol name="P398DLP_PUSHBUTTON2_SYM">
<pin name="A"/>
<pin name="B"/>
<pin name="C"/>
<pin name="D"/>
</symbol>
<symbol name="P398DLP_1XAAA_BATTERY_HOLDER_SYM">
<pin name="P$-"/>
<pin name="P$+"/>
</symbol>
<symbol name="P398DLP_RADIOFEATHER_M0_SYM">
<description>Adafruit RadioFeather M0 processor</description>
<pin name="RST"/>
<pin name="3V"/>
<pin name="AREF"/>
<pin name="GND"/>
<pin name="A0/#14"/>
<pin name="A1/#15"/>
<pin name="A2/#16"/>
<pin name="A3/#17"/>
<pin name="A4/#18"/>
<pin name="A5/#19"/>
<pin name="SCK/#24"/>
<pin name="MOSI/#23"/>
<pin name="MISO/#22"/>
<pin name="RX/#0"/>
<pin name="TX/#1"/>
<pin name="IO1"/>
<pin name="SDA/#20"/>
<pin name="SCL/#21"/>
<pin name="#5"/>
<pin name="#6"/>
<pin name="#9"/>
<pin name="#10"/>
<pin name="#11"/>
<pin name="#12"/>
<pin name="#13"/>
<pin name="USB"/>
<pin name="EN"/>
<pin name="BAT"/>
</symbol>
<symbol name="P398DLP_74HC137N_SYM">
<description>74HC137 1-of-8 demux</description>
<pin name="Y2BAR" direction="out"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="Y4BAR" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="OE1BAR" direction="in"/>
<pin name="Y5BAR" direction="in"/>
<pin name="Y6BAR" direction="in"/>
<pin name="OE0" direction="in"/>
<pin name="LE" direction="in"/>
<pin name="Y1BAR" direction="out"/>
<pin name="Y0BAR" direction="out"/>
<pin name="GND"/>
<pin name="VCC"/>
<pin name="Y3BAR" direction="out"/>
<pin name="Y7BAR" direction="in"/>
</symbol>
<symbol name="P398DLP_TTL_SERIAL_CAMERA_SYM">
<description>PAM8302A PWM audio amplifier</description>
<pin name="CVBS" direction="out"/>
<pin name="5V"/>
<pin name="TX" direction="out"/>
<pin name="RX" direction="in"/>
<pin name="GND"/>
</symbol>
<symbol name="P398DLP_ROSEGRAPHIC_SYM">
<description>VL53L0X proximity sensor</description>
</symbol>
<symbol name="P398DLP_RCA_PCB_JACK_SYM">
<description>pushbutton</description>
<pin name="PIN2" direction="pas" function="dot"/>
<pin name="PIN1B" direction="pas" function="dot"/>
<pin name="PIN1A" direction="pas" function="dot"/>
</symbol>
<symbol name="P398DLP_SPDT_SWITCH_SYM">
<description>ON/OFF/ON/OFF SPDT pushbutton</description>
<pin name="PIN1" direction="pas" function="dot"/>
<pin name="PIN2" direction="pas" function="dot"/>
<pin name="PIN3" direction="pas" function="dot"/>
</symbol>
<symbol name="P398DLP_GAS_SENSOR_SYM">
<description>Gas Sensors - MQ-3, MQ-4, MQ-6, MQ-7, MQ-8.
Through-hole gas sensors with a heating coil and an analog output.
MQ-3 = alcohol (red plastic case)
MQ-4 = methane CNG (wire mesh)
MQ-6 = LPG (wire mesh)
MQ-7 = CO (red plastic case)
MQ-8 = hydrogen (wire mesh)</description>
<pin name="A1"/>
<pin name="HA"/>
<pin name="B1"/>
<pin name="HB"/>
<pin name="A2"/>
<pin name="B2"/>
</symbol>
<symbol name="P398DLP_AP2112_SYM">
<pin name="VIN"/>
<pin name="GND"/>
<pin name="EN"/>
<pin name="NC"/>
<pin name="VOUT"/>
</symbol>
<symbol name="DIL18">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
</symbol>
<symbol name="DIL18-1">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
</symbol>
<symbol name="P398DLP_MCP23008_SYM">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
</symbol>
<symbol name="P398DLP_1N5817_SYM">
<description>1N5817 Schottky barrier diode</description>
<pin name="C"/>
<pin name="A"/>
</symbol>
<symbol name="SCHOTTKY">
<pin name="A" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="P398DLP_TPS7133Q_SYM">
<description>TPS7133Q 3.3V regulator</description>
<pin name="GND" direction="pas"/>
<pin name="ENBAR" direction="pas"/>
<pin name="IN1" direction="pas"/>
<pin name="IN2" direction="pas"/>
<pin name="OUT2" direction="pas"/>
<pin name="OUT1" direction="pas"/>
<pin name="SENSE/FB" direction="pas"/>
<pin name="PG" direction="pas"/>
</symbol>
<symbol name="P398DLP_AIRLIFT_SYM">
<description>Adafruit AirLift WiFi module</description>
<pin name="VIN" direction="pwr" function="dot"/>
<pin name="3VO" direction="pas" function="dot"/>
<pin name="GND" direction="pas" function="dot"/>
<pin name="SCK" direction="pas" function="dot"/>
<pin name="MISO" direction="pas" function="dot"/>
<pin name="MOSI" direction="pas" function="dot"/>
<pin name="CS" direction="pas" function="dot"/>
<pin name="BUSY" direction="pas" function="dot"/>
<pin name="RSTBAR" direction="pas" function="dot"/>
<pin name="RXI" direction="pas" function="dot"/>
<pin name="GP0" direction="pas" function="dot"/>
<pin name="TXO" direction="pas" function="dot"/>
</symbol>
<symbol name="P398DLP_TSOP38238_SYM">
<description>TSOP38238 IR receiver, 38 kHz</description>
<pin name="1_OUT"/>
<pin name="2_GND"/>
<pin name="3_VCC"/>
</symbol>
<symbol name="P398DLP_MOUNTING_HOLE_SYM">
<description>0.1 inch mounting hole</description>
</symbol>
<symbol name="P398DLP_MOLEX_DUAL_USB-A_SYM">
<description>molex 67298 dual USB-A,
vertically stacked</description>
<pin name="D-TOP"/>
<pin name="D+TOP"/>
<pin name="VBUSTOP"/>
<pin name="GNDTOP"/>
<pin name="D-BOT"/>
<pin name="D+BOT"/>
<pin name="VBUSBOT"/>
<pin name="GNDBOT"/>
</symbol>
<symbol name="P398DLP_FRAM_SYM">
<description>32kB FRAM I2C memory</description>
<pin name="VCC"/>
<pin name="GND"/>
<pin name="WP"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="A2"/>
<pin name="A1"/>
<pin name="A0"/>
</symbol>
<symbol name="P398DLP_ADG436_SWITCH_SYM">
<description>ADG436 dual SPDT analog switch</description>
<pin name="VDD" direction="out"/>
<pin name="IN1"/>
<pin name="S1A"/>
<pin name="D2" direction="in"/>
<pin name="D1"/>
<pin name="VSS" direction="in"/>
<pin name="S2A" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="GND" direction="in"/>
<pin name="S1B"/>
<pin name="NC3" direction="out"/>
<pin name="NC4" direction="out"/>
<pin name="NC2"/>
<pin name="NC5"/>
<pin name="S2B" direction="out"/>
<pin name="NC1" direction="in"/>
</symbol>
<symbol name="P398DLP_JUMPER_SYM">
<description>2 pin jumper</description>
<pin name="PIN1" direction="pas" function="dot"/>
<pin name="PIN2" direction="pas" function="dot"/>
</symbol>
<symbol name="P398DLP_SLIDE_SWITCH_SYM">
<description>slide switch, 0.3" through hole digikey KG01ET</description>
<pin name="PIN1" direction="pas" function="dot"/>
<pin name="PIN2" direction="pas" function="dot"/>
</symbol>
<symbol name="P398DLP_FEATHER_M4_EXPRESS_SYM">
<description>uit Feather M4 Express with samd51 processor</description>
<pin name="RST"/>
<pin name="3V"/>
<pin name="AREF"/>
<pin name="GND"/>
<pin name="A0/#14"/>
<pin name="A1/#15"/>
<pin name="A2/#16"/>
<pin name="A3/#17"/>
<pin name="A4/#18"/>
<pin name="A5/#19"/>
<pin name="SCK/#25"/>
<pin name="MOSI/#24"/>
<pin name="MISO/#23"/>
<pin name="RX/#0"/>
<pin name="TX/#1"/>
<pin name="D4/#4"/>
<pin name="SDA/#22"/>
<pin name="SCL/#21"/>
<pin name="#5"/>
<pin name="#6"/>
<pin name="#9"/>
<pin name="#10"/>
<pin name="#11"/>
<pin name="#12"/>
<pin name="#13"/>
<pin name="USB"/>
<pin name="EN"/>
<pin name="BAT"/>
</symbol>
<symbol name="P398DLP_MOLEX_USB-A_SYM">
<description>molex female USB-A 67643-3910</description>
<pin name="D-"/>
<pin name="D+"/>
<pin name="5V" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="P398DLP_RESISTOR_SIP7_SYM">
<description>4607X-101 SIP 6 resistor array</description>
<pin name="P$1"/>
<pin name="P$2"/>
<pin name="P$3"/>
<pin name="P$4"/>
<pin name="P$5"/>
<pin name="P$6"/>
<pin name="P$7"/>
</symbol>
<symbol name="P398DLP_MOUNTING_HOLE_4MM_SYM">
</symbol>
<symbol name="P398DLP_ARDUINO_MEGA2560_SYM">
<description>Arduino MEGA 2560, component side DOWN</description>
<pin name="SCL1" direction="pas" function="dot"/>
<pin name="SDA1" direction="pas" function="dot"/>
<pin name="AREF" direction="pas" function="dot"/>
<pin name="GND3" direction="pas" function="dot"/>
<pin name="D13" direction="pas" function="dot"/>
<pin name="D12" direction="pas" function="dot"/>
<pin name="D11" direction="pas" function="dot"/>
<pin name="D10" direction="pas" function="dot"/>
<pin name="D9" direction="pas" function="dot"/>
<pin name="D8" direction="pas" function="dot"/>
<pin name="D7" direction="pas" function="dot"/>
<pin name="D6" direction="pas" function="dot"/>
<pin name="D5" direction="pas" function="dot"/>
<pin name="D4" direction="pas" function="dot"/>
<pin name="D3" direction="pas" function="dot"/>
<pin name="D2" direction="pas" function="dot"/>
<pin name="D1&lt;-TX" direction="pas" function="dot"/>
<pin name="D0-&gt;RX" direction="pas" function="dot"/>
<pin name="D14TX3" direction="pas" function="dot"/>
<pin name="D15RX3" direction="pas" function="dot"/>
<pin name="D16TX2" direction="pas" function="dot"/>
<pin name="D17RX2" direction="pas" function="dot"/>
<pin name="D18TX1" direction="pas" function="dot"/>
<pin name="D19RX1" direction="pas" function="dot"/>
<pin name="D20SDA" direction="pas" function="dot"/>
<pin name="D21SCL" direction="pas" function="dot"/>
<pin name="NC" direction="pas" function="dot"/>
<pin name="IOREF" direction="pas" function="dot"/>
<pin name="RESET" direction="pas" function="dot"/>
<pin name="3.3V" direction="pas" function="dot"/>
<pin name="5V1" direction="pas" function="dot"/>
<pin name="GND1" direction="pas" function="dot"/>
<pin name="GND2" direction="pas" function="dot"/>
<pin name="VIN" direction="pas" function="dot"/>
<pin name="A0" direction="pas" function="dot"/>
<pin name="A1" direction="pas" function="dot"/>
<pin name="A2" direction="pas" function="dot"/>
<pin name="A3" direction="pas" function="dot"/>
<pin name="A4" direction="pas" function="dot"/>
<pin name="A5" direction="pas" function="dot"/>
<pin name="A6" direction="pas" function="dot"/>
<pin name="A7" direction="pas" function="dot"/>
<pin name="A8" direction="pas" function="dot"/>
<pin name="A9" direction="pas" function="dot"/>
<pin name="A10" direction="pas" function="dot"/>
<pin name="A11" direction="pas" function="dot"/>
<pin name="A12" direction="pas" function="dot"/>
<pin name="A13" direction="pas" function="dot"/>
<pin name="A14" direction="pas" function="dot"/>
<pin name="A15" direction="pas" function="dot"/>
<pin name="GND4" direction="pas" function="dot"/>
<pin name="GND5" direction="pas" function="dot"/>
<pin name="D52" direction="pas" function="dot"/>
<pin name="D53" direction="pas" function="dot"/>
<pin name="D50" direction="pas" function="dot"/>
<pin name="D51" direction="pas" function="dot"/>
<pin name="D48" direction="pas" function="dot"/>
<pin name="D49" direction="pas" function="dot"/>
<pin name="D46" direction="pas" function="dot"/>
<pin name="D47" direction="pas" function="dot"/>
<pin name="D44" direction="pas" function="dot"/>
<pin name="D45" direction="pas" function="dot"/>
<pin name="D42" direction="pas" function="dot"/>
<pin name="D43" direction="pas" function="dot"/>
<pin name="D40" direction="pas" function="dot"/>
<pin name="D41" direction="pas" function="dot"/>
<pin name="D38" direction="pas" function="dot"/>
<pin name="D39" direction="pas" function="dot"/>
<pin name="D36" direction="pas" function="dot"/>
<pin name="D37" direction="pas" function="dot"/>
<pin name="D34" direction="pas" function="dot"/>
<pin name="D35" direction="pas" function="dot"/>
<pin name="D32" direction="pas" function="dot"/>
<pin name="D33" direction="pas" function="dot"/>
<pin name="D30" direction="pas" function="dot"/>
<pin name="D31" direction="pas" function="dot"/>
<pin name="D28" direction="pas" function="dot"/>
<pin name="D29" direction="pas" function="dot"/>
<pin name="D26" direction="pas" function="dot"/>
<pin name="D27" direction="pas" function="dot"/>
<pin name="D24" direction="pas" function="dot"/>
<pin name="D25" direction="pas" function="dot"/>
<pin name="D22" direction="pas" function="dot"/>
<pin name="D23" direction="pas" function="dot"/>
<pin name="5V2" direction="pas" function="dot"/>
<pin name="5V3" direction="pas" function="dot"/>
</symbol>
<symbol name="PP398DLP_SPST_SWITCH_SYM">
<pin name="PIN1" direction="pas" function="dot"/>
<pin name="PIN2" direction="pas" function="dot"/>
<pin name="PIN3" direction="pas" function="dot"/>
</symbol>
<symbol name="P398DLP_SPST_SWITCH_SYM">
<description>Adafruit 1683 SPST ON/OFF switch</description>
<pin name="PIN1" direction="pas" function="dot"/>
<pin name="PIN2" direction="pas" function="dot"/>
</symbol>
<symbol name="P398DLP_LORA_BREAKOUT_SYM">
<description>LoRa 915 MHz breakout, Adafruit 3072</description>
<pin name="VIN" direction="pas" function="dot"/>
<pin name="GND" direction="pas" function="dot"/>
<pin name="EN" direction="pas" function="dot"/>
<pin name="G0" direction="pas" function="dot"/>
<pin name="SCK" direction="pas" function="dot"/>
<pin name="MISO" direction="pas" function="dot"/>
<pin name="MOSI" direction="pas" function="dot"/>
<pin name="CS" direction="pas" function="dot"/>
<pin name="RST" direction="pas" function="dot"/>
<pin name="G1" direction="pas" function="dot"/>
<pin name="G2" direction="pas" function="dot"/>
<pin name="G3" direction="pas" function="dot"/>
<pin name="G4" direction="pas" function="dot"/>
<pin name="G5" direction="pas" function="dot"/>
</symbol>
<symbol name="P398DLP_SPDT_SWITCH_2MM_SYM">
<description>SPDT slide switch, 2mm pitch: CKSwitches.com, OS102011MS2QN1</description>
<pin name="PIN1" direction="pas" function="dot"/>
<pin name="PIN2" direction="pas" function="dot"/>
<pin name="PIN3" direction="pas" function="dot"/>
</symbol>
<symbol name="PP398DLP_IN5817-B_SYM">
<pin name="A" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="P398DLP_BLUETOOTH_FRIEND_SYM">
<pin name="SCK"/>
<pin name="MISO"/>
<pin name="MOSI"/>
<pin name="CS"/>
<pin name="IRQ"/>
<pin name="DFU"/>
<pin name="RST"/>
<pin name="GND"/>
<pin name="VIN"/>
</symbol>
<symbol name="P398DLP_MICS5524_CO_SYM">
<description>MiCS5524 CO, Alcohol, and BVOC gas sensor
Adafruit 3199</description>
<pin name="5V"/>
<pin name="GND"/>
<pin name="AO"/>
<pin name="ENBAR"/>
</symbol>
<symbol name="P398DLP_PULSE_SENSOR_SYM">
<description>WorldFamousElectronics pulse sensor</description>
<pin name="GND"/>
<pin name="VDD"/>
<pin name="PULSE"/>
</symbol>
<symbol name="P398DLP_BME680_STEMMA_SYM">
<description>BME680 T/P/RH/VOC STEMMA connector</description>
<pin name="VIN"/>
<pin name="3V0"/>
<pin name="GND"/>
<pin name="SCK"/>
<pin name="SDO"/>
<pin name="SDI"/>
<pin name="CS"/>
</symbol>
<symbol name="P398DLP_2XAA_BATTERY_SYM">
<description>2xAA battery holder</description>
<pin name="BATTERY_3V" direction="pwr" function="dot"/>
<pin name="BATTERY_GND" direction="pwr" function="dot"/>
</symbol>
<symbol name="P398DLP_SPDT_DIP_SLIDE_SWITCH_SYM">
<description>SPDT slide switch, .098 inch pitch: EG1218 E-SWITCH, Adafruit 805</description>
<pin name="PIN1" direction="pas" function="dot"/>
<pin name="PIN2" direction="pas" function="dot"/>
<pin name="PIN3" direction="pas" function="dot"/>
</symbol>
<symbol name="P398DLP_MOUNTING_HOLE_300MIL_SYM">
<description>0.3 inch hole</description>
</symbol>
<symbol name="P398DLP_BQ24074_SOLAR_CHARGER_SYM">
<description>Adafruit bq24074 solar power charger: part ID 4755</description>
<pin name="VBUS"/>
<pin name="GND"/>
<pin name="THERM"/>
<pin name="ISET"/>
<pin name="CE"/>
<pin name="PGOOD"/>
<pin name="CHG"/>
<pin name="OUT"/>
<pin name="GND1"/>
<pin name="LIPO"/>
<pin name="GND2"/>
<pin name="D+"/>
<pin name="D-"/>
</symbol>
<symbol name="P398DLP_USB_MICRO_BREAKOUT_SYM">
<description>Adafruit 1833 microUSB breakout</description>
<pin name="GND"/>
<pin name="ID"/>
<pin name="D+"/>
<pin name="D-"/>
<pin name="5V"/>
</symbol>
<symbol name="P398DLP_MOUNTING_HOLE_250MIL_SYM">
<description>0.25 inch hole</description>
</symbol>
<symbol name="P398DLP_USB_C_BREAKOUT_SYM">
<description>Adafruit 4090 USB-C breakout</description>
<pin name="CC2"/>
<pin name="SBU1"/>
<pin name="D+"/>
<pin name="D-"/>
<pin name="CC1"/>
<pin name="SBU2"/>
<pin name="VBUS"/>
<pin name="GND"/>
</symbol>
<symbol name="P398DLP_VOLTMETER_SYM">
<description>Adafruit 2-wire voltmeter</description>
<pin name="GND" direction="pas" function="dot"/>
<pin name="VCC" direction="pas" function="dot"/>
</symbol>
<symbol name="P398DLP_ADC_QUAD_I2C_SYM">
<description>Adafruit "ultimate GPS" breakout board</description>
<pin name="GND" direction="pas" function="dot"/>
<pin name="SCL" direction="pas" function="dot"/>
<pin name="SDA" direction="pas" function="dot"/>
<pin name="ADDR" direction="pas" function="dot"/>
<pin name="ALRT" direction="pas" function="dot"/>
<pin name="A0" direction="pas" function="dot"/>
<pin name="A1" direction="pas" function="dot"/>
<pin name="A2" direction="pas" function="dot"/>
<pin name="A3" direction="pas" function="dot"/>
<pin name="VDD" direction="pas" function="dot"/>
</symbol>
<symbol name="P398DLP_DPS310_SYM">
<description>DPS310 precision pressure and temperature sensor. Adafruit 4494</description>
<pin name="VIN"/>
<pin name="3VO"/>
<pin name="GND"/>
<pin name="SCK"/>
<pin name="SDO"/>
<pin name="SDI"/>
<pin name="CS"/>
</symbol>
<symbol name="6P">
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="P398DLP_MCP4728_SYM">
<description>MCP4728 quad 12-bit DAC Adafriuit 4470</description>
<pin name="VCC"/>
<pin name="GND"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="LDAC"/>
<pin name="RDY"/>
<pin name="VCC2"/>
<pin name="VD"/>
<pin name="VC"/>
<pin name="VB"/>
<pin name="VA"/>
<pin name="GND2"/>
</symbol>
<symbol name="P398DLP_AS7262_SYM">
<description>AS7262 6-channel visible light sensor. Adafruit 3779</description>
<pin name="3V3"/>
<pin name="GND"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="RST"/>
<pin name="INT"/>
<pin name="LED"/>
<pin name="NC1"/>
<pin name="RX"/>
<pin name="TX"/>
<pin name="VIN2"/>
<pin name="NC2"/>
<pin name="VIN"/>
<pin name="GND2"/>
</symbol>
<symbol name="P398DLP_NPN_SYM">
<description>NPN transistor, TO-92 case</description>
<pin name="C"/>
<pin name="B"/>
<pin name="E"/>
</symbol>
<symbol name="P398DLP_SONY_SPRESENSE_EXTENSION_SYM">
<description>Sony Spresense extension board</description>
<pin name="D15" direction="pas" function="dot"/>
<pin name="D14" direction="pas" function="dot"/>
<pin name="AREF" direction="pas" function="dot"/>
<pin name="GND3" direction="pas" function="dot"/>
<pin name="D13" direction="pas" function="dot"/>
<pin name="D12" direction="pas" function="dot"/>
<pin name="D11" direction="pas" function="dot"/>
<pin name="D10" direction="pas" function="dot"/>
<pin name="D09" direction="pas" function="dot"/>
<pin name="D08" direction="pas" function="dot"/>
<pin name="D07" direction="pas" function="dot"/>
<pin name="D06" direction="pas" function="dot"/>
<pin name="D05" direction="pas" function="dot"/>
<pin name="D04" direction="pas" function="dot"/>
<pin name="D03" direction="pas" function="dot"/>
<pin name="D02" direction="pas" function="dot"/>
<pin name="D01&lt;-TX" direction="pas" function="dot"/>
<pin name="D00-&gt;RX" direction="pas" function="dot"/>
<pin name="RESERVE1" direction="pas" function="dot"/>
<pin name="IOREF" direction="pas" function="dot"/>
<pin name="RESET" direction="pas" function="dot"/>
<pin name="3.3V" direction="pas" function="dot"/>
<pin name="5V1" direction="pas" function="dot"/>
<pin name="GND1" direction="pas" function="dot"/>
<pin name="GND2" direction="pas" function="dot"/>
<pin name="RESERVE2" direction="pas" function="dot"/>
<pin name="A0" direction="pas" function="dot"/>
<pin name="A1" direction="pas" function="dot"/>
<pin name="A2" direction="pas" function="dot"/>
<pin name="A3" direction="pas" function="dot"/>
<pin name="A4" direction="pas" function="dot"/>
<pin name="A5" direction="pas" function="dot"/>
<pin name="D01_"/>
<pin name="D00_"/>
<pin name="D28_"/>
<pin name="D27_"/>
<pin name="D26_"/>
<pin name="D25_"/>
<pin name="D24_"/>
<pin name="D23_"/>
<pin name="3.3V1_"/>
<pin name="1.8V_"/>
<pin name="GND4_"/>
<pin name="D15_"/>
<pin name="GND5_"/>
<pin name="D16_"/>
<pin name="D17_"/>
<pin name="D18_"/>
<pin name="D19_"/>
<pin name="D20_"/>
<pin name="D21_"/>
<pin name="EXT_VDD"/>
<pin name="1.8V2_"/>
<pin name="XRST_PIN_1.8V"/>
<pin name="D14_"/>
<pin name="D22_"/>
<pin name="A2_"/>
<pin name="A3_"/>
</symbol>
<symbol name="P398DLP_MLX90640_CAMERA_SYM">
<description>MLX90640 low resolution IR camera. Adafruit 4407</description>
<pin name="VIN"/>
<pin name="3VO"/>
<pin name="GND"/>
<pin name="SCL"/>
<pin name="SDA"/>
</symbol>
<symbol name="P398DLP_RED_LED_SYM">
<description>red led</description>
<pin name="NEG" direction="pas" function="dot"/>
<pin name="POS" direction="pas" function="dot"/>
</symbol>
<symbol name="P398DLP_ROTARY_SWITCH_SYM">
<description>CTSCORP.com rotary switch
220ADC16</description>
<pin name="1"/>
<pin name="C1"/>
<pin name="4"/>
<pin name="2"/>
<pin name="C2"/>
<pin name="8"/>
</symbol>
<symbol name="P398DLP_ROSE4_SYM">
<description>rose bitmap graphic</description>
</symbol>
<symbol name="P398DLP_TFT_DISPLAY_SYM">
<description>160x128 TFT display</description>
<pin name="GND"/>
<pin name="VCC"/>
<pin name="RESET"/>
<pin name="D/C"/>
<pin name="CARD_CS"/>
<pin name="TFT_CS"/>
<pin name="MOSI"/>
<pin name="SCK"/>
<pin name="MISO"/>
<pin name="LITE"/>
</symbol>
<symbol name="P398DLP_LC709203F_STEMMA_SYM">
<description>LC709203F LiPo "fuel gauge"</description>
<pin name="VIN"/>
<pin name="GND"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="INT"/>
<pin name="THERM"/>
</symbol>
<symbol name="P398DLP_PUSHBUTTON2A_SYM">
<description>pushbutton, normally open</description>
<pin name="A"/>
<pin name="B"/>
<pin name="C"/>
<pin name="D"/>
</symbol>
<symbol name="P398DLP_AS7341_SYM">
<description>AS7341 10 channel spectrometer</description>
<pin name="GND"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="GPIO"/>
<pin name="INT"/>
<pin name="VIN"/>
</symbol>
<symbol name="P398DLP_PHOTO_INTERRUPTER_SYM">
<description>Adafruit four-wire photo interrupter</description>
<pin name="VCC" direction="pas" function="dot"/>
<pin name="LED" direction="pas" function="dot"/>
<pin name="OUT" direction="pas" function="dot"/>
<pin name="GND" direction="pas" function="dot"/>
</symbol>
<symbol name="P398DLP_SFM3300_HEADER_SYM">
<description>Sensirion SFM3300 flowmeter header</description>
<pin name="HEAT"/>
<pin name="SDA"/>
<pin name="GND"/>
<pin name="SCK"/>
<pin name="VDD"/>
<pin name="HEAT_GND"/>
</symbol>
<symbol name="P398DLP_DC_DC_CONVERTER_SYM">
<description>RECOM ROE SIP4 DC-DC converter
3,3 V to 5 V
ROE-3..305S part number</description>
<pin name="NEG_VIN"/>
<pin name="POS_VIN"/>
<pin name="NEG_VOUT"/>
<pin name="POS_VOUT"/>
</symbol>
<symbol name="P398DLP_L4931_REG_SYM">
<description>L4931 linear voltage regulator, TO-92 case
5.0V, adafruit 2236</description>
<pin name="VOUT"/>
<pin name="VIN"/>
<pin name="GND"/>
</symbol>
<symbol name="P398DLP_MAX30102_SPARKFUN_SYM">
<description>SparkFun Max30102 board
P398DLP_MAX30102_SPARKFUN</description>
<pin name="SCL_BOT" function="dot"/>
<pin name="SDA_BOT" function="dot"/>
<pin name="3V3_BOT" direction="pas" function="dot"/>
<pin name="GND_BOT" direction="pas" function="dot"/>
<pin name="SCL_TOP" direction="pas" function="dot"/>
<pin name="SDA_TOP" direction="pas" function="dot"/>
<pin name="3V3_TOP" direction="pas" function="dot"/>
<pin name="GND_TOP" direction="pas" function="dot"/>
</symbol>
<symbol name="P398DLP_ADXL375_SYM">
<description>ADXL375 200 g accelerometer</description>
<pin name="VIN" direction="pas" function="dot"/>
<pin name="3VO" direction="pas" function="dot"/>
<pin name="GND" direction="pas" function="dot"/>
<pin name="SCL" direction="pas" function="dot"/>
<pin name="SDA" direction="pas" function="dot"/>
<pin name="INT" direction="pas" function="dot"/>
<pin name="GND2" direction="pas" function="dot"/>
<pin name="I2" direction="pas" function="dot"/>
<pin name="SDO" direction="pas" function="dot"/>
<pin name="CS" direction="pas" function="dot"/>
</symbol>
<symbol name="P398DLP_H3LIS331_SYM">
<description>H3LIS331 400 g accelerometer</description>
<pin name="VIN" direction="pas" function="dot"/>
<pin name="3VO" direction="pas" function="dot"/>
<pin name="GND" direction="pas" function="dot"/>
<pin name="SCL" direction="pas" function="dot"/>
<pin name="SDA" direction="pas" function="dot"/>
<pin name="INT" direction="pas" function="dot"/>
<pin name="NC2" direction="pas" function="dot"/>
<pin name="NC3" direction="pas" function="dot"/>
<pin name="SDO" direction="pas" function="dot"/>
<pin name="CS" direction="pas" function="dot"/>
<pin name="NC1" direction="pas" function="dot"/>
<pin name="I2" direction="pas" function="dot"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="P398DLP_ADXL326_DEV" uservalue="yes">
<description>Adafruit ADXL326 3-axis accelerometer</description>
<gates>
<gate name="G$1" symbol="P398DLP_ADXL326_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_ADXL326_PKG">
<connects>
<connect gate="G$1" pin="3VO" pad="3VO"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="TEST" pad="TEST"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
<connect gate="G$1" pin="XOUT" pad="XOUT"/>
<connect gate="G$1" pin="YOUT" pad="YOUT"/>
<connect gate="G$1" pin="ZOUT" pad="ZOUT"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_BME680_DEV">
<description>BME680 temperature, pressure, relative humidity, and volatile organic compounds sensor</description>
<gates>
<gate name="G$1" symbol="P398DLP_BME680_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_BME680_PKG">
<connects>
<connect gate="G$1" pin="3V0" pad="2"/>
<connect gate="G$1" pin="CS" pad="7"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="SCK" pad="4"/>
<connect gate="G$1" pin="SDI" pad="6"/>
<connect gate="G$1" pin="SDO" pad="5"/>
<connect gate="G$1" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_DS3231_DEV">
<description>DS3231 real time clock with battery backup</description>
<gates>
<gate name="G$1" symbol="P398DLP_DS3231_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_DS3231_PKG">
<connects>
<connect gate="G$1" pin="32K" pad="6"/>
<connect gate="G$1" pin="BAT" pad="5"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="RSTBAR" pad="8"/>
<connect gate="G$1" pin="SCL" pad="3"/>
<connect gate="G$1" pin="SDA" pad="4"/>
<connect gate="G$1" pin="SQW" pad="7"/>
<connect gate="G$1" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_MCP4725_DEV">
<description>MCP4725 12-bit DAC</description>
<gates>
<gate name="G$1" symbol="P398DLP_MCP4725_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_MCP4725_PKG">
<connects>
<connect gate="G$1" pin="A0" pad="5"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="SCL" pad="3"/>
<connect gate="G$1" pin="SDA" pad="4"/>
<connect gate="G$1" pin="VDD" pad="1"/>
<connect gate="G$1" pin="VOUT" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_MICROSD_DEV">
<description>Adafruit microSD reader breakout board</description>
<gates>
<gate name="G$1" symbol="P398DLP_MICROSD_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_MICROSD_PKG">
<connects>
<connect gate="G$1" pin="3V" pad="2"/>
<connect gate="G$1" pin="5V" pad="1"/>
<connect gate="G$1" pin="CD" pad="8"/>
<connect gate="G$1" pin="CLK" pad="4"/>
<connect gate="G$1" pin="CS" pad="7"/>
<connect gate="G$1" pin="DI" pad="6"/>
<connect gate="G$1" pin="DO" pad="5"/>
<connect gate="G$1" pin="GND" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-1X7" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD7"/>
</gates>
<devices>
<device name="" package="1X07">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/90" package="1X07/90">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-1X3" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD3"/>
</gates>
<devices>
<device name="" package="1X03">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CB" package="1X03-CLEANBIG">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-1X4" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD4"/>
</gates>
<devices>
<device name="" package="1X04">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/90" package="1X04/90">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-1X5" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD5"/>
</gates>
<devices>
<device name="" package="1X05">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/90" package="1X05/90">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="5X2MM" package="1_05X2MM">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-1X6" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD6"/>
</gates>
<devices>
<device name="" package="1X06">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/90" package="1X06/90">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-1X8" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD8"/>
</gates>
<devices>
<device name="" package="1X08">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/90" package="1X08/90">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-1X9" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD9"/>
</gates>
<devices>
<device name="" package="1X09">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/90" package="1X09/90">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-1X10" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD10"/>
</gates>
<devices>
<device name="" package="1X10">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/90" package="1X10/90">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-1X11" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD11"/>
</gates>
<devices>
<device name="" package="1X11">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/90" package="1X11/90">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-1X12" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="PINHD12"/>
</gates>
<devices>
<device name="" package="1X12">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/90" package="1X12/90">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-2X18" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINH2X18"/>
</gates>
<devices>
<device name="" package="2X18">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="13" pad="13"/>
<connect gate="A" pin="14" pad="14"/>
<connect gate="A" pin="15" pad="15"/>
<connect gate="A" pin="16" pad="16"/>
<connect gate="A" pin="17" pad="17"/>
<connect gate="A" pin="18" pad="18"/>
<connect gate="A" pin="19" pad="19"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="20" pad="20"/>
<connect gate="A" pin="21" pad="21"/>
<connect gate="A" pin="22" pad="22"/>
<connect gate="A" pin="23" pad="23"/>
<connect gate="A" pin="24" pad="24"/>
<connect gate="A" pin="25" pad="25"/>
<connect gate="A" pin="26" pad="26"/>
<connect gate="A" pin="27" pad="27"/>
<connect gate="A" pin="28" pad="28"/>
<connect gate="A" pin="29" pad="29"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="30" pad="30"/>
<connect gate="A" pin="31" pad="31"/>
<connect gate="A" pin="32" pad="32"/>
<connect gate="A" pin="33" pad="33"/>
<connect gate="A" pin="34" pad="34"/>
<connect gate="A" pin="35" pad="35"/>
<connect gate="A" pin="36" pad="36"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/90" package="2X18/90">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="13" pad="13"/>
<connect gate="A" pin="14" pad="14"/>
<connect gate="A" pin="15" pad="15"/>
<connect gate="A" pin="16" pad="16"/>
<connect gate="A" pin="17" pad="17"/>
<connect gate="A" pin="18" pad="18"/>
<connect gate="A" pin="19" pad="19"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="20" pad="20"/>
<connect gate="A" pin="21" pad="21"/>
<connect gate="A" pin="22" pad="22"/>
<connect gate="A" pin="23" pad="23"/>
<connect gate="A" pin="24" pad="24"/>
<connect gate="A" pin="25" pad="25"/>
<connect gate="A" pin="26" pad="26"/>
<connect gate="A" pin="27" pad="27"/>
<connect gate="A" pin="28" pad="28"/>
<connect gate="A" pin="29" pad="29"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="30" pad="30"/>
<connect gate="A" pin="31" pad="31"/>
<connect gate="A" pin="32" pad="32"/>
<connect gate="A" pin="33" pad="33"/>
<connect gate="A" pin="34" pad="34"/>
<connect gate="A" pin="35" pad="35"/>
<connect gate="A" pin="36" pad="36"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-1X16" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD16"/>
</gates>
<devices>
<device name="" package="1X16">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="13" pad="13"/>
<connect gate="A" pin="14" pad="14"/>
<connect gate="A" pin="15" pad="15"/>
<connect gate="A" pin="16" pad="16"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/90" package="1X16/90">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="13" pad="13"/>
<connect gate="A" pin="14" pad="14"/>
<connect gate="A" pin="15" pad="15"/>
<connect gate="A" pin="16" pad="16"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TRIM_US-" prefix="R" uservalue="yes">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="POT_US-"/>
</gates>
<devices>
<device name="PT-10" package="PT-10">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="E" pad="E"/>
<connect gate="G$1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PT-10S" package="PT-10S">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="E" pad="E"/>
<connect gate="G$1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PT-SPIN" package="PT-SPIN">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="E" pad="E"/>
<connect gate="G$1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B25P" package="B25P">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="E" pad="E"/>
<connect gate="G$1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B25U" package="B25U">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="E" pad="E"/>
<connect gate="G$1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B25V" package="B25V">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="E" pad="E"/>
<connect gate="G$1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B25X" package="B25X">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="E" pad="E"/>
<connect gate="G$1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B64W" package="B64W">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="E" pad="E"/>
<connect gate="G$1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B64Y" package="B64Y">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="E" pad="E"/>
<connect gate="G$1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B90P" package="SP19L">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="E" pad="E"/>
<connect gate="G$1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CA6H" package="CA6H">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="E" pad="E"/>
<connect gate="G$1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CA6V" package="CA6V">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="E" pad="E"/>
<connect gate="G$1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CA9H" package="CA9H">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="E" pad="E"/>
<connect gate="G$1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CA9V" package="CA9V">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="E" pad="E"/>
<connect gate="G$1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CA14V" package="CA14V">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="E" pad="E"/>
<connect gate="G$1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CA14H" package="CA14H">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="E" pad="E"/>
<connect gate="G$1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CT6" package="CT6">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="E" pad="E"/>
<connect gate="G$1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ECP10P" package="ECP10P">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="E" pad="E"/>
<connect gate="G$1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ECP10S" package="ECP10S">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="E" pad="E"/>
<connect gate="G$1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LI10" package="LI10">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="E" pad="E"/>
<connect gate="G$1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LI15" package="LI15">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="E" pad="E"/>
<connect gate="G$1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RJ6" package="RJ6">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="E" pad="E"/>
<connect gate="G$1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RJ6S" package="RJ6S">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="E" pad="E"/>
<connect gate="G$1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RJ9W" package="RJ9W">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="E" pad="E"/>
<connect gate="G$1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RS3" package="RS3">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="E" pad="E"/>
<connect gate="G$1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S43P" package="SP19L">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="E" pad="E"/>
<connect gate="G$1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S63P" package="S63P">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="E" pad="E"/>
<connect gate="G$1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S63S" package="S63S">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="E" pad="E"/>
<connect gate="G$1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S63X" package="S63X">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="E" pad="E"/>
<connect gate="G$1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S64W" package="S64W">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="E" pad="E"/>
<connect gate="G$1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S64Y" package="S64Y">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="E" pad="E"/>
<connect gate="G$1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S75H" package="S75H">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="E" pad="E"/>
<connect gate="G$1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S75P" package="S75P">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="E" pad="E"/>
<connect gate="G$1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SP19L" package="SP19L">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="E" pad="E"/>
<connect gate="G$1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ST10" package="ST10">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="E" pad="E"/>
<connect gate="G$1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ST15" package="ST15">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="E" pad="E"/>
<connect gate="G$1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="T189" package="SP19LKN">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="E" pad="E"/>
<connect gate="G$1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PT10" package="PT-10">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="E" pad="E"/>
<connect gate="G$1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PT10S" package="PT-10S">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="E" pad="E"/>
<connect gate="G$1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTSPIN" package="PT-SPIN">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="E" pad="E"/>
<connect gate="G$1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CIP20C-4MM" package="CIP20C-4MM">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="E" pad="E"/>
<connect gate="G$1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CIP20C-6MM" package="CIP20C-6MM">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="E" pad="E"/>
<connect gate="G$1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SM-42/43A" package="SM-42/43A">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="E" pad="3"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SM-42/43X" package="SM-42/43X">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="E" pad="3"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SM-42/43W" package="SM-42/43W">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="E" pad="3"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SM-42/43B" package="SM-42/43B">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="E" pad="3"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3223G" package="3223G">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="E" pad="3"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3223J" package="3223J">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="E" pad="3"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3223W" package="3223W">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="E" pad="3"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_MICROPHONE_DEV">
<description>Adafruit amplified electret microphone</description>
<gates>
<gate name="G$1" symbol="P398DLP_MICROPHONE_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_MICROPHONE_PKG">
<connects>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="OUT" pad="OUT"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_ULTIMATE_GPS_DEV">
<description>Adafruit "ultimate GPS" breakout board</description>
<gates>
<gate name="G$1" symbol="P398DLP_ULTIMATE_GPS_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_ULTIMATE_GPS_PKG">
<connects>
<connect gate="G$1" pin="3.3V" pad="3.3V"/>
<connect gate="G$1" pin="EN" pad="EN"/>
<connect gate="G$1" pin="FIX" pad="FIX"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="PPS" pad="PPS"/>
<connect gate="G$1" pin="RX" pad="RX"/>
<connect gate="G$1" pin="TX" pad="TX"/>
<connect gate="G$1" pin="VBAT" pad="VBAT"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_SPEAKER_DEV">
<description>0.5 watt, 8 ohm mini-metal speaker</description>
<gates>
<gate name="G$1" symbol="P398DLP_SPEAKER_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_SPEAKER_PKG">
<connects>
<connect gate="G$1" pin="VIN+" pad="VIN+"/>
<connect gate="G$1" pin="VIN-" pad="VIN-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_PUSHBUTTON_DEV">
<description>pushbutton</description>
<gates>
<gate name="G$1" symbol="P398DLP_PUSHBUTTON_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_RCA_PCB_JACK_PKG">
<connects>
<connect gate="G$1" pin="NC" pad="PIN1B"/>
<connect gate="G$1" pin="PIN1" pad="PIN1A"/>
<connect gate="G$1" pin="PIN2" pad="PIN2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_INA219_DEV">
<description>INA219 current/voltage sensor</description>
<gates>
<gate name="G$1" symbol="P398DLP_INA219_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_INA219_PKG">
<connects>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="SCL" pad="SCL"/>
<connect gate="G$1" pin="SDA" pad="SDA"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
<connect gate="G$1" pin="VIN+" pad="VIN+"/>
<connect gate="G$1" pin="VIN-" pad="VIN-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_LCD_16X2_DEV">
<description>2x16 liquid crystal display, four mounting holes. Crystalfontz CFAH1602B-NGG-JTV</description>
<gates>
<gate name="G$1" symbol="P398DLP_LCD_16X2_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_LCD_16X2_PKG">
<connects>
<connect gate="G$1" pin="5V" pad="5V"/>
<connect gate="G$1" pin="DB0" pad="DB0"/>
<connect gate="G$1" pin="DB1" pad="DB1"/>
<connect gate="G$1" pin="DB2" pad="DB2"/>
<connect gate="G$1" pin="DB3" pad="DB3"/>
<connect gate="G$1" pin="DB4" pad="DB4"/>
<connect gate="G$1" pin="DB5" pad="DB5"/>
<connect gate="G$1" pin="DB6" pad="DB6"/>
<connect gate="G$1" pin="DB7" pad="DB7"/>
<connect gate="G$1" pin="E" pad="E"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="NC" pad="NC"/>
<connect gate="G$1" pin="PULL" pad="PULL"/>
<connect gate="G$1" pin="R/W" pad="R/W"/>
<connect gate="G$1" pin="RS" pad="RS"/>
<connect gate="G$1" pin="VO" pad="VO"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_KEYPAD_DEV">
<description>3x4 telephone-style keypad</description>
<gates>
<gate name="G$1" symbol="P398DLP_KEYPAD_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_KEYPAD_PKG">
<connects>
<connect gate="G$1" pin="COL1" pad="COL1"/>
<connect gate="G$1" pin="COL2" pad="COL2"/>
<connect gate="G$1" pin="COL3" pad="COL3"/>
<connect gate="G$1" pin="NC" pad="NC"/>
<connect gate="G$1" pin="ROW1" pad="ROW1"/>
<connect gate="G$1" pin="ROW2" pad="ROW2"/>
<connect gate="G$1" pin="ROW3" pad="ROW3"/>
<connect gate="G$1" pin="ROW4" pad="ROW4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_5XAA_BATTERY_DEV">
<description>5 x AA battery case</description>
<gates>
<gate name="G$1" symbol="P398DLP_5XAA_BATTERY_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_5XAA_BATTERY_PKG">
<connects>
<connect gate="G$1" pin="BATTERY_7.5V" pad="BATTERY_7.5V"/>
<connect gate="G$1" pin="BATTERY_GND" pad="BATTERY_GND"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-1X2" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="PINHD2-1"/>
</gates>
<devices>
<device name="" package="1X02">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/90" package="1X02/90">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-1X1" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="PINHD1"/>
</gates>
<devices>
<device name="" package="1X01">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_PAM8302A_DEV">
<description>PAM8302A PWM audio amplifier</description>
<gates>
<gate name="G$1" symbol="P398DLP_PAM8302A_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_PAM8302A_PKG">
<connects>
<connect gate="G$1" pin="A+" pad="A+"/>
<connect gate="G$1" pin="A-" pad="A-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="SD_BAR" pad="SD"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
<connect gate="G$1" pin="VO+" pad="VO+"/>
<connect gate="G$1" pin="VO-" pad="VO-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_TSL2561_DEV">
<description>TSL251 Lux Sensor</description>
<gates>
<gate name="G$1" symbol="P398DLP_TSL2561_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_TSL2561_PKG">
<connects>
<connect gate="G$1" pin="3.3V" pad="3.3V"/>
<connect gate="G$1" pin="ADDR" pad="ADDR"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="INT" pad="INT"/>
<connect gate="G$1" pin="SCL_5V" pad="SCL_5V"/>
<connect gate="G$1" pin="SDA_5V" pad="SDA_5V"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_GUVA_ANALOG_UV_DEV">
<description>GUVA analog UV</description>
<gates>
<gate name="G$1" symbol="P398DLP_GUVA_ANALOG_UV_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_GUVA_ANALOG_UV_PKG">
<connects>
<connect gate="G$1" pin="5.0V" pad="5.0V"/>
<connect gate="G$1" pin="AOUT" pad="AOUT"/>
<connect gate="G$1" pin="GND" pad="GND"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_ARDUINO_FLIPPED_DEV">
<description>Arduino MEGA 2560, components down</description>
<gates>
<gate name="G$1" symbol="P398DLP_ARDUINO_FLIPPED_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_ARDUINO_FLIPPED_PKG">
<connects>
<connect gate="G$1" pin="3.3V" pad="3.3V"/>
<connect gate="G$1" pin="5V1" pad="5V1"/>
<connect gate="G$1" pin="5V2" pad="5V2"/>
<connect gate="G$1" pin="5V3" pad="5V3"/>
<connect gate="G$1" pin="A0" pad="A0"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A10" pad="A10"/>
<connect gate="G$1" pin="A11" pad="A11"/>
<connect gate="G$1" pin="A12" pad="A12"/>
<connect gate="G$1" pin="A13" pad="A13"/>
<connect gate="G$1" pin="A14" pad="A14"/>
<connect gate="G$1" pin="A15" pad="A15"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="A6" pad="A6"/>
<connect gate="G$1" pin="A7" pad="A7"/>
<connect gate="G$1" pin="A8" pad="A8"/>
<connect gate="G$1" pin="A9" pad="A9"/>
<connect gate="G$1" pin="AREF" pad="AREF"/>
<connect gate="G$1" pin="BATTERY_7.5V" pad="BATTERY_7.5V"/>
<connect gate="G$1" pin="BATTERY_GND" pad="BATTERY_GND"/>
<connect gate="G$1" pin="D0-&gt;RX" pad="D0-&gt;RX"/>
<connect gate="G$1" pin="D10" pad="D10"/>
<connect gate="G$1" pin="D11" pad="D11"/>
<connect gate="G$1" pin="D12" pad="D12"/>
<connect gate="G$1" pin="D13" pad="D13"/>
<connect gate="G$1" pin="D14TX3" pad="D14TX3"/>
<connect gate="G$1" pin="D15RX3" pad="D15RX3"/>
<connect gate="G$1" pin="D16TX2" pad="D16TX2"/>
<connect gate="G$1" pin="D17RX2" pad="D17RX2"/>
<connect gate="G$1" pin="D18TX1" pad="D18TX1"/>
<connect gate="G$1" pin="D19RX1" pad="D19RX1"/>
<connect gate="G$1" pin="D1&lt;-TX" pad="D1&lt;-TX"/>
<connect gate="G$1" pin="D2" pad="D2"/>
<connect gate="G$1" pin="D20SDA" pad="D20SDA"/>
<connect gate="G$1" pin="D21SCL" pad="D21SCL"/>
<connect gate="G$1" pin="D22" pad="D22"/>
<connect gate="G$1" pin="D23" pad="D23"/>
<connect gate="G$1" pin="D24" pad="D24"/>
<connect gate="G$1" pin="D25" pad="D25"/>
<connect gate="G$1" pin="D26" pad="D26"/>
<connect gate="G$1" pin="D27" pad="D27"/>
<connect gate="G$1" pin="D28" pad="D28"/>
<connect gate="G$1" pin="D29" pad="D29"/>
<connect gate="G$1" pin="D3" pad="D3"/>
<connect gate="G$1" pin="D30" pad="D30"/>
<connect gate="G$1" pin="D31" pad="D31"/>
<connect gate="G$1" pin="D32" pad="D32"/>
<connect gate="G$1" pin="D33" pad="D33"/>
<connect gate="G$1" pin="D34" pad="D34"/>
<connect gate="G$1" pin="D35" pad="D35"/>
<connect gate="G$1" pin="D36" pad="D36"/>
<connect gate="G$1" pin="D37" pad="D37"/>
<connect gate="G$1" pin="D38" pad="D38"/>
<connect gate="G$1" pin="D39" pad="D39"/>
<connect gate="G$1" pin="D4" pad="D4"/>
<connect gate="G$1" pin="D40" pad="D40"/>
<connect gate="G$1" pin="D41" pad="D41"/>
<connect gate="G$1" pin="D42" pad="D42"/>
<connect gate="G$1" pin="D43" pad="D43"/>
<connect gate="G$1" pin="D44" pad="D44"/>
<connect gate="G$1" pin="D45" pad="D45"/>
<connect gate="G$1" pin="D46" pad="D46"/>
<connect gate="G$1" pin="D47" pad="D47"/>
<connect gate="G$1" pin="D48" pad="D48"/>
<connect gate="G$1" pin="D49" pad="D49"/>
<connect gate="G$1" pin="D5" pad="D5"/>
<connect gate="G$1" pin="D50" pad="D50"/>
<connect gate="G$1" pin="D51" pad="D51"/>
<connect gate="G$1" pin="D52" pad="D52"/>
<connect gate="G$1" pin="D53" pad="D53"/>
<connect gate="G$1" pin="D6" pad="D6"/>
<connect gate="G$1" pin="D7" pad="D7"/>
<connect gate="G$1" pin="D8" pad="D8"/>
<connect gate="G$1" pin="D9" pad="D9"/>
<connect gate="G$1" pin="GND1" pad="GND1"/>
<connect gate="G$1" pin="GND2" pad="GND2"/>
<connect gate="G$1" pin="GND3" pad="GND3"/>
<connect gate="G$1" pin="GND4" pad="GND4"/>
<connect gate="G$1" pin="GND5" pad="GND5"/>
<connect gate="G$1" pin="IOREF" pad="IOREF"/>
<connect gate="G$1" pin="NC" pad="NC"/>
<connect gate="G$1" pin="RESET" pad="RESET"/>
<connect gate="G$1" pin="SCL1" pad="SCL1"/>
<connect gate="G$1" pin="SDA1" pad="SDA1"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
<connect gate="G$1" pin="_A0" pad="A0_"/>
<connect gate="G$1" pin="_A1" pad="A1_"/>
<connect gate="G$1" pin="_A10" pad="A10_"/>
<connect gate="G$1" pin="_A11" pad="A11_"/>
<connect gate="G$1" pin="_A12" pad="A12_"/>
<connect gate="G$1" pin="_A13" pad="A13_"/>
<connect gate="G$1" pin="_A14" pad="A14_"/>
<connect gate="G$1" pin="_A15" pad="A15_"/>
<connect gate="G$1" pin="_A2" pad="A2_"/>
<connect gate="G$1" pin="_A3" pad="A3_"/>
<connect gate="G$1" pin="_A4" pad="A4_"/>
<connect gate="G$1" pin="_A5" pad="A5_"/>
<connect gate="G$1" pin="_A6" pad="A6_"/>
<connect gate="G$1" pin="_A7" pad="A7_"/>
<connect gate="G$1" pin="_A8" pad="A8_"/>
<connect gate="G$1" pin="_A9" pad="A9_"/>
<connect gate="G$1" pin="_AREF" pad="AREF_"/>
<connect gate="G$1" pin="_D0-&gt;RX" pad="D0-&gt;RX_"/>
<connect gate="G$1" pin="_D10" pad="D10_"/>
<connect gate="G$1" pin="_D11" pad="D11_"/>
<connect gate="G$1" pin="_D12" pad="D12_"/>
<connect gate="G$1" pin="_D13" pad="D13_"/>
<connect gate="G$1" pin="_D14TX3" pad="D14TX3_"/>
<connect gate="G$1" pin="_D15RX3" pad="D15RX3_"/>
<connect gate="G$1" pin="_D16TX2" pad="DX16TX2_"/>
<connect gate="G$1" pin="_D17RX2" pad="D17RX2_"/>
<connect gate="G$1" pin="_D18TX1" pad="D18TX1_"/>
<connect gate="G$1" pin="_D19RX1" pad="D19RX1_"/>
<connect gate="G$1" pin="_D1&lt;-TX" pad="D1&lt;-TX_"/>
<connect gate="G$1" pin="_D2" pad="D2_"/>
<connect gate="G$1" pin="_D20SDA" pad="D20SDA_"/>
<connect gate="G$1" pin="_D21SCL" pad="D21SCL_"/>
<connect gate="G$1" pin="_D23" pad="D23_"/>
<connect gate="G$1" pin="_D24" pad="D24_"/>
<connect gate="G$1" pin="_D25" pad="D25_"/>
<connect gate="G$1" pin="_D26" pad="D26_"/>
<connect gate="G$1" pin="_D27" pad="D27_"/>
<connect gate="G$1" pin="_D28" pad="D28_"/>
<connect gate="G$1" pin="_D29" pad="D29_"/>
<connect gate="G$1" pin="_D3" pad="D3_"/>
<connect gate="G$1" pin="_D30" pad="D30_"/>
<connect gate="G$1" pin="_D31" pad="D31_"/>
<connect gate="G$1" pin="_D32" pad="D32_"/>
<connect gate="G$1" pin="_D33" pad="D33_"/>
<connect gate="G$1" pin="_D34" pad="D34_"/>
<connect gate="G$1" pin="_D35" pad="D35_"/>
<connect gate="G$1" pin="_D36" pad="D36_"/>
<connect gate="G$1" pin="_D37" pad="D37_"/>
<connect gate="G$1" pin="_D38" pad="D38_"/>
<connect gate="G$1" pin="_D39" pad="D39_"/>
<connect gate="G$1" pin="_D4" pad="D4_"/>
<connect gate="G$1" pin="_D40" pad="D40_"/>
<connect gate="G$1" pin="_D41" pad="D41_"/>
<connect gate="G$1" pin="_D42" pad="D42_"/>
<connect gate="G$1" pin="_D43" pad="D43_"/>
<connect gate="G$1" pin="_D44" pad="D44_"/>
<connect gate="G$1" pin="_D45" pad="D45_"/>
<connect gate="G$1" pin="_D46" pad="D46_"/>
<connect gate="G$1" pin="_D47" pad="D47_"/>
<connect gate="G$1" pin="_D48" pad="D48_"/>
<connect gate="G$1" pin="_D49" pad="D49_"/>
<connect gate="G$1" pin="_D5" pad="D5_"/>
<connect gate="G$1" pin="_D51" pad="D51_"/>
<connect gate="G$1" pin="_D53" pad="D53_"/>
<connect gate="G$1" pin="_D6" pad="D6_"/>
<connect gate="G$1" pin="_D7" pad="D7_"/>
<connect gate="G$1" pin="_D8" pad="D8_"/>
<connect gate="G$1" pin="_D9" pad="D9_"/>
<connect gate="G$1" pin="_IOREF" pad="IOREF_"/>
<connect gate="G$1" pin="_RESET" pad="RESET_"/>
<connect gate="G$1" pin="_SCL1" pad="SCL1_"/>
<connect gate="G$1" pin="_SDA1" pad="SDA1_"/>
<connect gate="G$1" pin="_VIN" pad="VIN_"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_VL53L0X_DEV">
<description>VL53L0X proximity sensor</description>
<gates>
<gate name="G$1" symbol="P398DLP_VL53L0X_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_VL53L0X_PKG">
<connects>
<connect gate="G$1" pin="2V8" pad="2V8"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GPIO" pad="GPIO"/>
<connect gate="G$1" pin="SCL" pad="SCL"/>
<connect gate="G$1" pin="SDA" pad="SDA"/>
<connect gate="G$1" pin="SHDN" pad="SHDN"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_L3GD20H_DEV">
<description>L3GD20H three axis gyro</description>
<gates>
<gate name="G$1" symbol="P398DLP_L3GD20H_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_L3GD20H_PKG">
<connects>
<connect gate="G$1" pin="3VOUT" pad="3VOUT"/>
<connect gate="G$1" pin="CS" pad="CS"/>
<connect gate="G$1" pin="DRDY" pad="DRDY"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="INT1" pad="INT1"/>
<connect gate="G$1" pin="SA0" pad="SA0"/>
<connect gate="G$1" pin="SCL" pad="SCL"/>
<connect gate="G$1" pin="SDA" pad="SDA"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_ON-OFF-ON-OFF_SWITCH_DEV">
<description>on-off-on-off pushbutton switch</description>
<gates>
<gate name="G$1" symbol="P398DLP_ON-OFF-ON-OFF_SWITCH_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_ON-OFF-ON-OFF_SWITCH_PKG">
<connects>
<connect gate="G$1" pin="CENTER" pad="CENTER"/>
<connect gate="G$1" pin="LEFT" pad="LEFT"/>
<connect gate="G$1" pin="RIGHT" pad="RIGHT"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_TRIMPOT_DEV">
<description>trimpot</description>
<gates>
<gate name="G$1" symbol="P398DLP_TRIMPOT_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_TRIMPOT_PKG">
<connects>
<connect gate="G$1" pin="BOTTOM" pad="BOTTOM"/>
<connect gate="G$1" pin="TAP" pad="TAP"/>
<connect gate="G$1" pin="TOP" pad="TOP"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_MLX90614_IR_DEV">
<description>MLX90614 non-contact IR thermometer</description>
<gates>
<gate name="G$1" symbol="P398DLP_MLX90614_IR_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_MLX90614_IR_PKG">
<connects>
<connect gate="G$1" pin="PWM/SDA" pad="2"/>
<connect gate="G$1" pin="SCL/VZ" pad="1"/>
<connect gate="G$1" pin="VDD" pad="3"/>
<connect gate="G$1" pin="VSS" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_LSM9DS1_9DOF_DEV">
<description>LSM9DS1 9 DOF accelerometer/gyro/magnetometer</description>
<gates>
<gate name="G$1" symbol="P398DLP_LSM9DS1_9DOF_SYM"/>
</gates>
<devices>
<device name="LSM" package="P398DLP_LSM9DS1_9DOF_PKG">
<connects>
<connect gate="G$1" pin="3V3" pad="3V3"/>
<connect gate="G$1" pin="CSAG" pad="CSAG"/>
<connect gate="G$1" pin="CSM" pad="CSM"/>
<connect gate="G$1" pin="DEN" pad="DEN"/>
<connect gate="G$1" pin="DRDY" pad="DRDY"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="INT1" pad="INT1"/>
<connect gate="G$1" pin="INT2" pad="INT2"/>
<connect gate="G$1" pin="INTM" pad="INTM"/>
<connect gate="G$1" pin="SCL" pad="SCL"/>
<connect gate="G$1" pin="SDA" pad="SDA"/>
<connect gate="G$1" pin="SDOAG" pad="SDOAG"/>
<connect gate="G$1" pin="SDOM" pad="SDOM"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_MMA8451_ACCEL_DEV">
<description>MMA8451 3 axis accelerometer</description>
<gates>
<gate name="G$1" symbol="P398DLP_MMA8451_ACCEL_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_MMA8451_ACCEL_PKG">
<connects>
<connect gate="G$1" pin="3VO" pad="3VO"/>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="I1" pad="I1"/>
<connect gate="G$1" pin="I2" pad="I2"/>
<connect gate="G$1" pin="SCL" pad="SCL"/>
<connect gate="G$1" pin="SDA" pad="SDA"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_FORCE_SENSITIVE_RESISTOR_DEV">
<description>force sensitive resistor</description>
<gates>
<gate name="G$1" symbol="P398DLP_FORCE_SENSITIVE_RESISTOR_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_FORCE_SENSITIVE_RESISTOR_PKG">
<connects>
<connect gate="G$1" pin="5V/FSR1" pad="5V/FSR1"/>
<connect gate="G$1" pin="FSR2" pad="FSR2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_ANEMOMETER_DEV">
<description>anemometer</description>
<gates>
<gate name="G$1" symbol="P398DLP_ANEMOMETER_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_ANEMOMETER_PKG">
<connects>
<connect gate="G$1" pin="7.5V" pad="7.5V"/>
<connect gate="G$1" pin="ANEMOMETER" pad="ANEMOMETER"/>
<connect gate="G$1" pin="GND" pad="GND"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_MYOWARE_DEV">
<description>myoware EMG sensor</description>
<gates>
<gate name="G$1" symbol="P398DLP_MYOWARE_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_MYOWARE_PKG">
<connects>
<connect gate="G$1" pin="5V" pad="5V"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="MYOWARE" pad="MYOWARE"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_GP2Y0A21YK0F_IR_PROXIMITY_DEV">
<description>IR proximity sensor</description>
<gates>
<gate name="G$1" symbol="P398DLP_GP2Y0A21YK0F_IR_PROXIMITY_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_GP2Y0A21YK0F_IR_PROXIMITY_PKG">
<connects>
<connect gate="G$1" pin="5V" pad="5V"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="IR_PROXIMITY" pad="IR_PROXIMITY"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_POWER+ADC_DEV">
<description>ADC + power + ground</description>
<gates>
<gate name="G$1" symbol="P398DLP_POWER+ADC_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_POWER+ADC_PKG">
<connects>
<connect gate="G$1" pin="5V" pad="5V"/>
<connect gate="G$1" pin="ADC" pad="ADC"/>
<connect gate="G$1" pin="GND" pad="GND"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_PMS5003_PM2.5_DEV">
<description>PMS5003 PM2.5 particulates sensor</description>
<gates>
<gate name="G$1" symbol="P398DLP_PMS5003_PM2.5_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_PMS5003_PM2.5_PKG">
<connects>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="NC1" pad="NC1"/>
<connect gate="G$1" pin="NC2" pad="NC2"/>
<connect gate="G$1" pin="RST" pad="RST"/>
<connect gate="G$1" pin="RXD" pad="RXD"/>
<connect gate="G$1" pin="SET" pad="SET"/>
<connect gate="G$1" pin="TXD" pad="TXD"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_TCA9548A_MUX_DEV">
<description>TCA9548A I2C MUX</description>
<gates>
<gate name="G$1" symbol="P398DLP_TCA9548A_MUX_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_TCA9548A_MUX_PKG">
<connects>
<connect gate="G$1" pin="A0" pad="A0"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="RST" pad="RST"/>
<connect gate="G$1" pin="SC0" pad="SC0"/>
<connect gate="G$1" pin="SC1" pad="SC1"/>
<connect gate="G$1" pin="SC2" pad="SC2"/>
<connect gate="G$1" pin="SC3" pad="SC3"/>
<connect gate="G$1" pin="SC4" pad="SC4"/>
<connect gate="G$1" pin="SC5" pad="SC5"/>
<connect gate="G$1" pin="SC6" pad="SC6"/>
<connect gate="G$1" pin="SC7" pad="SC7"/>
<connect gate="G$1" pin="SCL" pad="SCL"/>
<connect gate="G$1" pin="SD0" pad="SD0"/>
<connect gate="G$1" pin="SD1" pad="SD1"/>
<connect gate="G$1" pin="SD2" pad="SD2"/>
<connect gate="G$1" pin="SD3" pad="SD3"/>
<connect gate="G$1" pin="SD4" pad="SD4"/>
<connect gate="G$1" pin="SD5" pad="SD5"/>
<connect gate="G$1" pin="SD6" pad="SD6"/>
<connect gate="G$1" pin="SD7" pad="SD7"/>
<connect gate="G$1" pin="SDA" pad="SDA"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_DRV2605L_HAPTIC_DEV">
<description>DRV2605L haptic (vibrator) driver</description>
<gates>
<gate name="G$1" symbol="P398DLP_DRV2605L_HAPTIC_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_DRV2605L_HAPTIC_PKG">
<connects>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="IN" pad="IN"/>
<connect gate="G$1" pin="MOTOR+" pad="MOTOR+"/>
<connect gate="G$1" pin="MOTOR-" pad="MOTOR-"/>
<connect gate="G$1" pin="SCL" pad="SCL"/>
<connect gate="G$1" pin="SDA" pad="SDA"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_HAPTIC_VIBRATOR_MOTOR_DEV">
<description>haptic vibrator</description>
<gates>
<gate name="G$1" symbol="P398DLP_HAPTIC_VIBRATOR_MOTOR_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_HAPTIC_VIBRATOR_MOTOR_PKG">
<connects>
<connect gate="G$1" pin="MOTOR+" pad="MOTOR+"/>
<connect gate="G$1" pin="MOTOR-" pad="MOTOR-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_POWER+I2C_SYM">
<description>powered I2C connection</description>
<gates>
<gate name="G$2" symbol="P398DLP_POWER+I2C_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_POWER+I2C_PKG">
<connects>
<connect gate="G$2" pin="5V" pad="5V"/>
<connect gate="G$2" pin="GND" pad="GND"/>
<connect gate="G$2" pin="SCL" pad="SCL"/>
<connect gate="G$2" pin="SDA" pad="SDA"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_ADALOGGER_MO_DEV">
<description>Adafruit Adalogger M0 processor</description>
<gates>
<gate name="G$1" symbol="P398DLP_ADALOGGER_M0_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_ADALOGGER_M0_PKG">
<connects>
<connect gate="G$1" pin="#10" pad="#10"/>
<connect gate="G$1" pin="#11" pad="#11"/>
<connect gate="G$1" pin="#12" pad="#12"/>
<connect gate="G$1" pin="#13" pad="#13"/>
<connect gate="G$1" pin="#5" pad="#5"/>
<connect gate="G$1" pin="#6" pad="#6"/>
<connect gate="G$1" pin="#9" pad="#9"/>
<connect gate="G$1" pin="3V" pad="3V"/>
<connect gate="G$1" pin="A0" pad="A0"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="AREF" pad="AREF"/>
<connect gate="G$1" pin="BAT" pad="BAT"/>
<connect gate="G$1" pin="EN" pad="EN"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GND2" pad="GND2"/>
<connect gate="G$1" pin="MISO" pad="MISO/#22"/>
<connect gate="G$1" pin="MOSI" pad="MOSI/#23"/>
<connect gate="G$1" pin="RST" pad="RST"/>
<connect gate="G$1" pin="RX" pad="RX/#0"/>
<connect gate="G$1" pin="SCK" pad="SCK/#24"/>
<connect gate="G$1" pin="SCL" pad="SCL/#21"/>
<connect gate="G$1" pin="SDA" pad="SDA/#20"/>
<connect gate="G$1" pin="TX" pad="TX/#1"/>
<connect gate="G$1" pin="USB" pad="USB"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_74HC157N_DEV">
<description>74HC157N quad mux</description>
<gates>
<gate name="G$1" symbol="P398DLP_74HC157N_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_74HC157N_PKG">
<connects>
<connect gate="G$1" pin="!A!/B" pad="ABAR/B"/>
<connect gate="G$1" pin="1A" pad="1A"/>
<connect gate="G$1" pin="1B" pad="1B"/>
<connect gate="G$1" pin="1Y" pad="1Y"/>
<connect gate="G$1" pin="2A" pad="2A"/>
<connect gate="G$1" pin="2B" pad="2B"/>
<connect gate="G$1" pin="2Y" pad="2Y"/>
<connect gate="G$1" pin="3A" pad="3A"/>
<connect gate="G$1" pin="3B" pad="3B"/>
<connect gate="G$1" pin="3Y" pad="3Y"/>
<connect gate="G$1" pin="4A" pad="4A"/>
<connect gate="G$1" pin="4B" pad="4B"/>
<connect gate="G$1" pin="4Y" pad="4Y"/>
<connect gate="G$1" pin="G" pad="GBAR"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_PUSHBUTTON2_DEV">
<description>pushbutton, normally open</description>
<gates>
<gate name="G$1" symbol="P398DLP_PUSHBUTTON2_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_PUSHBUTTON2_PKG">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$1" pin="D" pad="D"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_1XAAA_BATTERY_HOLDER_DEV">
<description>eagle plastics 1xAAA battery holder, part # 12BH411P-R-GR</description>
<gates>
<gate name="G$1" symbol="P398DLP_1XAAA_BATTERY_HOLDER_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_1XAAA_BATTERY_HOLDER_PKG">
<connects>
<connect gate="G$1" pin="P$+" pad="PIN+"/>
<connect gate="G$1" pin="P$-" pad="PIN-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_RADIOFEATHER_MO_DEV">
<description>Adafruit RadioFeather M0 processor</description>
<gates>
<gate name="G$1" symbol="P398DLP_RADIOFEATHER_M0_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_RADIOFEATHER_M0_PKG">
<connects>
<connect gate="G$1" pin="#10" pad="#10"/>
<connect gate="G$1" pin="#11" pad="#11"/>
<connect gate="G$1" pin="#12" pad="#12"/>
<connect gate="G$1" pin="#13" pad="#13"/>
<connect gate="G$1" pin="#5" pad="#5"/>
<connect gate="G$1" pin="#6" pad="#6"/>
<connect gate="G$1" pin="#9" pad="#9"/>
<connect gate="G$1" pin="3V" pad="3V"/>
<connect gate="G$1" pin="A0/#14" pad="A0/#14"/>
<connect gate="G$1" pin="A1/#15" pad="A1/#15"/>
<connect gate="G$1" pin="A2/#16" pad="A2/#16"/>
<connect gate="G$1" pin="A3/#17" pad="A3/#17"/>
<connect gate="G$1" pin="A4/#18" pad="A4/#18"/>
<connect gate="G$1" pin="A5/#19" pad="A5/#19"/>
<connect gate="G$1" pin="AREF" pad="AREF"/>
<connect gate="G$1" pin="BAT" pad="BAT"/>
<connect gate="G$1" pin="EN" pad="EN"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="IO1" pad="IO1"/>
<connect gate="G$1" pin="MISO/#22" pad="MISO/#22"/>
<connect gate="G$1" pin="MOSI/#23" pad="MOSI/#23"/>
<connect gate="G$1" pin="RST" pad="RST"/>
<connect gate="G$1" pin="RX/#0" pad="RX/#0"/>
<connect gate="G$1" pin="SCK/#24" pad="SCK/#24"/>
<connect gate="G$1" pin="SCL/#21" pad="SCL/#21"/>
<connect gate="G$1" pin="SDA/#20" pad="SDA/#20"/>
<connect gate="G$1" pin="TX/#1" pad="TX/#1"/>
<connect gate="G$1" pin="USB" pad="USB"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_74HC137N_DEV">
<description>74HC137N 1-of-8 demux</description>
<gates>
<gate name="G$1" symbol="P398DLP_74HC137N_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_74HC137N_PKG">
<connects>
<connect gate="G$1" pin="A0" pad="A0"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="LE" pad="LE"/>
<connect gate="G$1" pin="OE0" pad="OE0"/>
<connect gate="G$1" pin="OE1BAR" pad="OE1BAR"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
<connect gate="G$1" pin="Y0BAR" pad="Y0BAR"/>
<connect gate="G$1" pin="Y1BAR" pad="Y1BAR"/>
<connect gate="G$1" pin="Y2BAR" pad="Y2BAR"/>
<connect gate="G$1" pin="Y3BAR" pad="Y3BAR"/>
<connect gate="G$1" pin="Y4BAR" pad="Y4BAR"/>
<connect gate="G$1" pin="Y5BAR" pad="Y5BAR"/>
<connect gate="G$1" pin="Y6BAR" pad="Y6BAR"/>
<connect gate="G$1" pin="Y7BAR" pad="Y7BAR"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_TTL_SERIAL_CAMERA_DEV">
<description>VC0706 TTL Serial Camera</description>
<gates>
<gate name="G$1" symbol="P398DLP_TTL_SERIAL_CAMERA_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_TTL_SERIAL_CAMERA_PKG">
<connects>
<connect gate="G$1" pin="5V" pad="5V"/>
<connect gate="G$1" pin="CVBS" pad="CVBS"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="RX" pad="RX"/>
<connect gate="G$1" pin="TX" pad="TX"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_ROSEGRAPHIC_DEV">
<description>VL53L0X proximity sensor</description>
<gates>
<gate name="G$1" symbol="P398DLP_VL53L0X_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_VL53L0X_PKG">
<connects>
<connect gate="G$1" pin="2V8" pad="2V8"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GPIO" pad="GPIO"/>
<connect gate="G$1" pin="SCL" pad="SCL"/>
<connect gate="G$1" pin="SDA" pad="SDA"/>
<connect gate="G$1" pin="SHDN" pad="SHDN"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_RCA_PCB_JACK_DEV">
<description>RCA PCB jack.
Digi-key CP-1409-ND,
Manufacturer RCJ-024</description>
<gates>
<gate name="G$1" symbol="P398DLP_RCA_PCB_JACK_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_RCA_PCB_JACK_PKG">
<connects>
<connect gate="G$1" pin="PIN1A" pad="PIN1A"/>
<connect gate="G$1" pin="PIN1B" pad="PIN1B"/>
<connect gate="G$1" pin="PIN2" pad="PIN2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_SPDT_SWITCH_DEV">
<description>SPDT PCB toggle switch</description>
<gates>
<gate name="G$1" symbol="P398DLP_SPDT_SWITCH_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_SPDT_SWITCH_PKG">
<connects>
<connect gate="G$1" pin="PIN1" pad="PIN1"/>
<connect gate="G$1" pin="PIN2" pad="PIN2"/>
<connect gate="G$1" pin="PIN3" pad="PIN3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_GAS_SENSOR_DEV" prefix="GS">
<description>&lt;h3&gt;Gas Sensors - MQ-3, MQ-4, MQ-6, MQ-7, MQ-8&lt;/h3&gt;
&lt;p&gt;Through-hole gas sensors with a heating coil and an analog output.&lt;/p&gt;
&lt;p&gt;&lt;a href="https://cdn.sparkfun.com/datasheets/Sensors/Biometric/MQ-3%20ver1.3%20-%20Manual.pdf"&gt;Example Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/8891"&gt;Gas Sensor Breakout Board&lt;/a&gt; (BOB-8891) - Breakout board compatible with all gas sensors.&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/8880"&gt;Alcohol Gas Sensor - MQ-3&lt;/a&gt; (SEN-08880)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/9404"&gt;Methane CNG Gas Sensor - MQ-4&lt;/a&gt; (SEN-09404)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/9405"&gt;LPG Gas Sensor - MQ-6&lt;/a&gt; (SEN-09405)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/9403"&gt;Carbon Monoxide Sensor - MQ-7&lt;/a&gt; (SEN-09403)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/10916"&gt;Hydrogen Gas Sensor - MQ-8&lt;/a&gt; (SEN-10916)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="P398DLP_GAS_SENSOR_SYM"/>
</gates>
<devices>
<device name="MQ-3" package="P398DLP_GAS_SENSOR_PKG">
<connects>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="B1" pad="B1"/>
<connect gate="G$1" pin="B2" pad="B2"/>
<connect gate="G$1" pin="HA" pad="HA"/>
<connect gate="G$1" pin="HB" pad="HB"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="COMP-12216"/>
<attribute name="SF_ID" value="SEN-08880"/>
</technology>
</technologies>
</device>
<device name="MQ-4" package="P398DLP_GAS_SENSOR_PKG">
<connects>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="B1" pad="B1"/>
<connect gate="G$1" pin="B2" pad="B2"/>
<connect gate="G$1" pin="HA" pad="HA"/>
<connect gate="G$1" pin="HB" pad="HB"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="COMP-11559"/>
<attribute name="SF_ID" value="SEN-09404"/>
</technology>
</technologies>
</device>
<device name="MQ-6" package="P398DLP_GAS_SENSOR_PKG">
<connects>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="B1" pad="B1"/>
<connect gate="G$1" pin="B2" pad="B2"/>
<connect gate="G$1" pin="HA" pad="HA"/>
<connect gate="G$1" pin="HB" pad="HB"/>
</connects>
<technologies>
<technology name="">
<attribute name="SF_ID" value="SEN-09405"/>
</technology>
</technologies>
</device>
<device name="MQ-7" package="P398DLP_GAS_SENSOR_PKG">
<connects>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="B1" pad="B1"/>
<connect gate="G$1" pin="B2" pad="B2"/>
<connect gate="G$1" pin="HA" pad="HA"/>
<connect gate="G$1" pin="HB" pad="HB"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="COMP-12214"/>
<attribute name="SF_ID" value="SEN-09403"/>
</technology>
</technologies>
</device>
<device name="MQ-8" package="P398DLP_GAS_SENSOR_PKG">
<connects>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="B1" pad="B1"/>
<connect gate="G$1" pin="B2" pad="B2"/>
<connect gate="G$1" pin="HA" pad="HA"/>
<connect gate="G$1" pin="HB" pad="HB"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="COMP-13351"/>
<attribute name="SF_ID" value="SEN-10916"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_AP2112_DEV">
<description>AP2112 SOT25 package LDO 3.3 V regulator with enable</description>
<gates>
<gate name="G$1" symbol="P398DLP_AP2112_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_AP2112_PKG">
<connects>
<connect gate="G$1" pin="EN" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="NC" pad="4"/>
<connect gate="G$1" pin="VIN" pad="1"/>
<connect gate="G$1" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DIL18" prefix="IC" uservalue="yes">
<description>&lt;b&gt;Dual In Line / Socket&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="DIL18-1"/>
</gates>
<devices>
<device name="" package="DIL18">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="POPULARITY" value="1"/>
</technology>
</technologies>
</device>
<device name="S" package="SOCKET-18">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="POPULARITY" value="0"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_MCP23008_DEV" prefix="IC" uservalue="yes">
<description>MCP23008 I2C port extender</description>
<gates>
<gate name="G$1" symbol="P398DLP_MCP23008_SYM"/>
</gates>
<devices>
<device name="P398DLP_MCP23008_PKG1" package="P398DLP_MCP23008_PKG">
<connects>
<connect gate="G$1" pin="1" pad="SCL"/>
<connect gate="G$1" pin="10" pad="GP0"/>
<connect gate="G$1" pin="11" pad="GP1"/>
<connect gate="G$1" pin="12" pad="GP2"/>
<connect gate="G$1" pin="13" pad="GP3"/>
<connect gate="G$1" pin="14" pad="GP4"/>
<connect gate="G$1" pin="15" pad="GP5"/>
<connect gate="G$1" pin="16" pad="GP6"/>
<connect gate="G$1" pin="17" pad="GP7"/>
<connect gate="G$1" pin="18" pad="VDD"/>
<connect gate="G$1" pin="2" pad="SDA"/>
<connect gate="G$1" pin="3" pad="A2"/>
<connect gate="G$1" pin="4" pad="A1"/>
<connect gate="G$1" pin="5" pad="A0"/>
<connect gate="G$1" pin="6" pad="RESETBAR"/>
<connect gate="G$1" pin="7" pad="NC"/>
<connect gate="G$1" pin="8" pad="INT"/>
<connect gate="G$1" pin="9" pad="GND"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_1N5817_DEV">
<description>1N5817 Schottky barrier diode</description>
<gates>
<gate name="G$1" symbol="P398DLP_1N5817_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_1N5817_PKG">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="1N581*" prefix="D">
<description>&lt;b&gt;1.0A SCHOTTKY BARRIER RECTIFIER&lt;/b&gt;&lt;p&gt;
Source: http://www.diodes.com/datasheets/ds23001.pdf</description>
<gates>
<gate name="G$1" symbol="SCHOTTKY"/>
</gates>
<devices>
<device name="" package="DO41-7.6">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="7-B">
<attribute name="POPULARITY" value="0"/>
</technology>
<technology name="7-T">
<attribute name="POPULARITY" value="0"/>
</technology>
<technology name="8-B">
<attribute name="POPULARITY" value="0"/>
</technology>
<technology name="8-T">
<attribute name="POPULARITY" value="0"/>
</technology>
<technology name="9-B">
<attribute name="POPULARITY" value="11"/>
</technology>
<technology name="9-T">
<attribute name="POPULARITY" value="0"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_TPS7133Q_DEV">
<description>3.3V regulator with enable.</description>
<gates>
<gate name="G$1" symbol="P398DLP_TPS7133Q_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_TPS7133Q_PKG">
<connects>
<connect gate="G$1" pin="ENBAR" pad="ENBAR"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="IN1" pad="IN1"/>
<connect gate="G$1" pin="IN2" pad="IN2"/>
<connect gate="G$1" pin="OUT1" pad="OUT1"/>
<connect gate="G$1" pin="OUT2" pad="OUT2"/>
<connect gate="G$1" pin="PG" pad="PG"/>
<connect gate="G$1" pin="SENSE/FB" pad="SENSE/FB"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_AIRLIFT_DEV" uservalue="yes">
<description>Adafruit AirLift WiFi module (part 4201)</description>
<gates>
<gate name="G$1" symbol="P398DLP_AIRLIFT_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_AIRLIFT_PKG">
<connects>
<connect gate="G$1" pin="3VO" pad="3VO"/>
<connect gate="G$1" pin="BUSY" pad="BUSY"/>
<connect gate="G$1" pin="CS" pad="CS"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GP0" pad="GP0"/>
<connect gate="G$1" pin="MISO" pad="MISO"/>
<connect gate="G$1" pin="MOSI" pad="MOSI"/>
<connect gate="G$1" pin="RSTBAR" pad="RSTBAR"/>
<connect gate="G$1" pin="RXI" pad="RXI"/>
<connect gate="G$1" pin="SCK" pad="SCK"/>
<connect gate="G$1" pin="TXO" pad="TXO"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_TSOP38238_DEV">
<description>TSOP38238 IR receiver, 38 kHz</description>
<gates>
<gate name="G$1" symbol="P398DLP_TSOP38238_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_TSOP38238_PKG">
<connects>
<connect gate="G$1" pin="1_OUT" pad="1"/>
<connect gate="G$1" pin="2_GND" pad="2"/>
<connect gate="G$1" pin="3_VCC" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_MOUNTING_HOLE_DEV">
<description>0.1 inch mounting hole</description>
<gates>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_MOLEX_USB-A_DEV">
<description>USB-A female connector, molex 67643-3910</description>
<gates>
<gate name="G$1" symbol="P398DLP_MOLEX_USB-A_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_MOLEX_USB-A_PKG">
<connects>
<connect gate="G$1" pin="5V" pad="1"/>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_FRAM_DEV">
<description>32kB FRAM I2C memory</description>
<gates>
<gate name="G$1" symbol="P398DLP_FRAM_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_FRAM_PKG">
<connects>
<connect gate="G$1" pin="A0" pad="8"/>
<connect gate="G$1" pin="A1" pad="7"/>
<connect gate="G$1" pin="A2" pad="6"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="SCL" pad="4"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="VCC" pad="1"/>
<connect gate="G$1" pin="WP" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_ADG436_SWITCH_DEV">
<description>ADG436 dual analog SPDT switch</description>
<gates>
<gate name="G$1" symbol="P398DLP_ADG436_SWITCH_SYM"/>
</gates>
<devices>
<device name="ADG" package="P398DLP_ADG436_SWITCH_PKG">
<connects>
<connect gate="G$1" pin="D1" pad="D1"/>
<connect gate="G$1" pin="D2" pad="D2"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="IN1" pad="IN1"/>
<connect gate="G$1" pin="IN2" pad="IN2"/>
<connect gate="G$1" pin="NC1" pad="NC1"/>
<connect gate="G$1" pin="NC2" pad="NC2"/>
<connect gate="G$1" pin="NC3" pad="NC3"/>
<connect gate="G$1" pin="NC4" pad="NC4"/>
<connect gate="G$1" pin="NC5" pad="NC5"/>
<connect gate="G$1" pin="S1A" pad="S1A"/>
<connect gate="G$1" pin="S1B" pad="S1B"/>
<connect gate="G$1" pin="S2A" pad="S2A"/>
<connect gate="G$1" pin="S2B" pad="S2B"/>
<connect gate="G$1" pin="VDD" pad="VDD"/>
<connect gate="G$1" pin="VSS" pad="VSS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_JUMPER_DEV">
<description>2 pin jumper</description>
<gates>
<gate name="G$1" symbol="P398DLP_JUMPER_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_JUMPER_PKG">
<connects>
<connect gate="G$1" pin="PIN1" pad="PIN1"/>
<connect gate="G$1" pin="PIN2" pad="PIN2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_SLIDE_SWITCH_DEV">
<description>slide switch, 0.3" through hole
digikey KG01ET</description>
<gates>
<gate name="G$1" symbol="P398DLP_SLIDE_SWITCH_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_SLIDE_SWITCH_PKG">
<connects>
<connect gate="G$1" pin="PIN1" pad="PIN1"/>
<connect gate="G$1" pin="PIN2" pad="PIN2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_FEATHER_M4_EXPRESS_DEV">
<description>Adafruit Feather M4 Express with samd51 processor</description>
<gates>
<gate name="G$1" symbol="P398DLP_FEATHER_M4_EXPRESS_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_FEATHER_M4_EXPRESS_PKG">
<connects>
<connect gate="G$1" pin="#10" pad="#10"/>
<connect gate="G$1" pin="#11" pad="#11"/>
<connect gate="G$1" pin="#12" pad="#12"/>
<connect gate="G$1" pin="#13" pad="#13"/>
<connect gate="G$1" pin="#5" pad="#5"/>
<connect gate="G$1" pin="#6" pad="#6"/>
<connect gate="G$1" pin="#9" pad="#9"/>
<connect gate="G$1" pin="3V" pad="3V"/>
<connect gate="G$1" pin="A0/#14" pad="A0/#14"/>
<connect gate="G$1" pin="A1/#15" pad="A1/#15"/>
<connect gate="G$1" pin="A2/#16" pad="A2/#16"/>
<connect gate="G$1" pin="A3/#17" pad="A3/#17"/>
<connect gate="G$1" pin="A4/#18" pad="A4/#18"/>
<connect gate="G$1" pin="A5/#19" pad="A5/#19"/>
<connect gate="G$1" pin="AREF" pad="AREF"/>
<connect gate="G$1" pin="BAT" pad="BAT"/>
<connect gate="G$1" pin="D4/#4" pad="D4/#4"/>
<connect gate="G$1" pin="EN" pad="EN"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="MISO/#23" pad="MISO/#23"/>
<connect gate="G$1" pin="MOSI/#24" pad="MOSI/#24"/>
<connect gate="G$1" pin="RST" pad="RST"/>
<connect gate="G$1" pin="RX/#0" pad="RX/#0"/>
<connect gate="G$1" pin="SCK/#25" pad="SCK/#25"/>
<connect gate="G$1" pin="SCL/#21" pad="SCL/#21"/>
<connect gate="G$1" pin="SDA/#22" pad="SDA/#22"/>
<connect gate="G$1" pin="TX/#1" pad="TX/#1"/>
<connect gate="G$1" pin="USB" pad="USB"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_MOLEX_DUAL_USB-A_DEV" uservalue="yes">
<description>molex dual female USB-A 67298</description>
<gates>
<gate name="G$1" symbol="P398DLP_MOLEX_DUAL_USB-A_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_MOLEX_DUAL_USB-A_PKG">
<connects>
<connect gate="G$1" pin="D+BOT" pad="7"/>
<connect gate="G$1" pin="D+TOP" pad="3"/>
<connect gate="G$1" pin="D-BOT" pad="6"/>
<connect gate="G$1" pin="D-TOP" pad="2"/>
<connect gate="G$1" pin="GNDBOT" pad="8"/>
<connect gate="G$1" pin="GNDTOP" pad="4"/>
<connect gate="G$1" pin="VBUSBOT" pad="5"/>
<connect gate="G$1" pin="VBUSTOP" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_RESISTOR_SIP7_DEV">
<description>Bourns 4607X-101 resistor array</description>
<gates>
<gate name="G$1" symbol="P398DLP_RESISTOR_SIP7_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_RESISTOR_SIP7_PKG">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
<connect gate="G$1" pin="P$2" pad="P$2"/>
<connect gate="G$1" pin="P$3" pad="P$3"/>
<connect gate="G$1" pin="P$4" pad="P$4"/>
<connect gate="G$1" pin="P$5" pad="P$5"/>
<connect gate="G$1" pin="P$6" pad="P$6"/>
<connect gate="G$1" pin="P$7" pad="P$7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_ARDUINO_MEGA2560_DEV">
<description>Arduino MEGA 2560, component side DOWN</description>
<gates>
<gate name="G$1" symbol="P398DLP_ARDUINO_MEGA2560_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_ARDUINO_MEGA2560_PKG">
<connects>
<connect gate="G$1" pin="3.3V" pad="3.3V"/>
<connect gate="G$1" pin="5V1" pad="5V1"/>
<connect gate="G$1" pin="5V2" pad="5V2"/>
<connect gate="G$1" pin="5V3" pad="5V3"/>
<connect gate="G$1" pin="A0" pad="A0"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A10" pad="A10"/>
<connect gate="G$1" pin="A11" pad="A11"/>
<connect gate="G$1" pin="A12" pad="A12"/>
<connect gate="G$1" pin="A13" pad="A13"/>
<connect gate="G$1" pin="A14" pad="A14"/>
<connect gate="G$1" pin="A15" pad="A15"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="A6" pad="A6"/>
<connect gate="G$1" pin="A7" pad="A7"/>
<connect gate="G$1" pin="A8" pad="A8"/>
<connect gate="G$1" pin="A9" pad="A9"/>
<connect gate="G$1" pin="AREF" pad="AREF"/>
<connect gate="G$1" pin="D0-&gt;RX" pad="D0-&gt;RX"/>
<connect gate="G$1" pin="D10" pad="D10"/>
<connect gate="G$1" pin="D11" pad="D11"/>
<connect gate="G$1" pin="D12" pad="D12"/>
<connect gate="G$1" pin="D13" pad="D13"/>
<connect gate="G$1" pin="D14TX3" pad="D14TX3"/>
<connect gate="G$1" pin="D15RX3" pad="D15RX3"/>
<connect gate="G$1" pin="D16TX2" pad="D16TX2"/>
<connect gate="G$1" pin="D17RX2" pad="D17RX2"/>
<connect gate="G$1" pin="D18TX1" pad="D18TX1"/>
<connect gate="G$1" pin="D19RX1" pad="D19RX1"/>
<connect gate="G$1" pin="D1&lt;-TX" pad="D1&lt;-TX"/>
<connect gate="G$1" pin="D2" pad="D2"/>
<connect gate="G$1" pin="D20SDA" pad="D20SDA"/>
<connect gate="G$1" pin="D21SCL" pad="D21SCL"/>
<connect gate="G$1" pin="D22" pad="D22"/>
<connect gate="G$1" pin="D23" pad="D23"/>
<connect gate="G$1" pin="D24" pad="D24"/>
<connect gate="G$1" pin="D25" pad="D25"/>
<connect gate="G$1" pin="D26" pad="D26"/>
<connect gate="G$1" pin="D27" pad="D27"/>
<connect gate="G$1" pin="D28" pad="D28"/>
<connect gate="G$1" pin="D29" pad="D29"/>
<connect gate="G$1" pin="D3" pad="D3"/>
<connect gate="G$1" pin="D30" pad="D30"/>
<connect gate="G$1" pin="D31" pad="D31"/>
<connect gate="G$1" pin="D32" pad="D32"/>
<connect gate="G$1" pin="D33" pad="D33"/>
<connect gate="G$1" pin="D34" pad="D34"/>
<connect gate="G$1" pin="D35" pad="D35"/>
<connect gate="G$1" pin="D36" pad="D36"/>
<connect gate="G$1" pin="D37" pad="D37"/>
<connect gate="G$1" pin="D38" pad="D38"/>
<connect gate="G$1" pin="D39" pad="D39"/>
<connect gate="G$1" pin="D4" pad="D4"/>
<connect gate="G$1" pin="D40" pad="D40"/>
<connect gate="G$1" pin="D41" pad="D41"/>
<connect gate="G$1" pin="D42" pad="D42"/>
<connect gate="G$1" pin="D43" pad="D43"/>
<connect gate="G$1" pin="D44" pad="D44"/>
<connect gate="G$1" pin="D45" pad="D45"/>
<connect gate="G$1" pin="D46" pad="D46"/>
<connect gate="G$1" pin="D47" pad="D47"/>
<connect gate="G$1" pin="D48" pad="D48"/>
<connect gate="G$1" pin="D49" pad="D49"/>
<connect gate="G$1" pin="D5" pad="D5"/>
<connect gate="G$1" pin="D50" pad="D50"/>
<connect gate="G$1" pin="D51" pad="D51"/>
<connect gate="G$1" pin="D52" pad="D52"/>
<connect gate="G$1" pin="D53" pad="D53"/>
<connect gate="G$1" pin="D6" pad="D6"/>
<connect gate="G$1" pin="D7" pad="D7"/>
<connect gate="G$1" pin="D8" pad="D8"/>
<connect gate="G$1" pin="D9" pad="D9"/>
<connect gate="G$1" pin="GND1" pad="GND1"/>
<connect gate="G$1" pin="GND2" pad="GND2"/>
<connect gate="G$1" pin="GND3" pad="GND3"/>
<connect gate="G$1" pin="GND4" pad="GND4"/>
<connect gate="G$1" pin="GND5" pad="GND5"/>
<connect gate="G$1" pin="IOREF" pad="IOREF"/>
<connect gate="G$1" pin="NC" pad="NC"/>
<connect gate="G$1" pin="RESET" pad="RESET"/>
<connect gate="G$1" pin="SCL1" pad="SCL1"/>
<connect gate="G$1" pin="SDA1" pad="SDA1"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_SPST_SWITCH_DEV">
<description>Adafruit 1683 SPST ON/OFF switch</description>
<gates>
<gate name="G$1" symbol="P398DLP_SPST_SWITCH_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_SPST_SWITCH_PKG">
<connects>
<connect gate="G$1" pin="PIN1" pad="A+"/>
<connect gate="G$1" pin="PIN2" pad="A-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_LORA_BREAKOUT_DEV">
<description>LoRa 915 MHz breakout, Adafruit 3072</description>
<gates>
<gate name="G$1" symbol="P398DLP_LORA_BREAKOUT_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_LORA_BREAKOUT_PKG">
<connects>
<connect gate="G$1" pin="CS" pad="CS"/>
<connect gate="G$1" pin="EN" pad="EN"/>
<connect gate="G$1" pin="G0" pad="G0"/>
<connect gate="G$1" pin="G1" pad="G1"/>
<connect gate="G$1" pin="G2" pad="G2"/>
<connect gate="G$1" pin="G3" pad="G3"/>
<connect gate="G$1" pin="G4" pad="G4"/>
<connect gate="G$1" pin="G5" pad="G5"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="MISO" pad="MISO/CIPO"/>
<connect gate="G$1" pin="MOSI" pad="MOSI/COPI"/>
<connect gate="G$1" pin="RST" pad="RST"/>
<connect gate="G$1" pin="SCK" pad="SCK"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_SPDT_SWITCH_2MM_DEV">
<description>SPDT slide switch, 2mm pitch: CKSwitches.com, OS102011MS2QN1</description>
<gates>
<gate name="G$1" symbol="P398DLP_SPDT_SWITCH_2MM_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_SPDT_SWITCH_2MM_PKG">
<connects>
<connect gate="G$1" pin="PIN1" pad="PIN1"/>
<connect gate="G$1" pin="PIN2" pad="PIN2"/>
<connect gate="G$1" pin="PIN3" pad="PIN3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_BLUETOOTH_FRIEND_DEV">
<description>Adafruit Bluetooth LE SPI friend: 2633</description>
<gates>
<gate name="G$1" symbol="P398DLP_BLUETOOTH_FRIEND_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_BLUETOOTH_FRIEND_PKG">
<connects>
<connect gate="G$1" pin="CS" pad="CS"/>
<connect gate="G$1" pin="DFU" pad="DFU"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="IRQ" pad="IRQ"/>
<connect gate="G$1" pin="MISO" pad="MISO"/>
<connect gate="G$1" pin="MOSI" pad="MOSI"/>
<connect gate="G$1" pin="RST" pad="RST"/>
<connect gate="G$1" pin="SCK" pad="SCK"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_MICS5524_CO_DEV">
<description>MiCS5524 CO, Alcohol, and VOC gas sensor
Adafruit 3199</description>
<gates>
<gate name="G$1" symbol="P398DLP_MICS5524_CO_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_MICS5524_CO_PKG">
<connects>
<connect gate="G$1" pin="5V" pad="5V"/>
<connect gate="G$1" pin="AO" pad="AO"/>
<connect gate="G$1" pin="ENBAR" pad="ENBAR"/>
<connect gate="G$1" pin="GND" pad="GND"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_PULSE_SENSOR_DEV">
<description>WorldFamousElectronics pulse sensor</description>
<gates>
<gate name="G$1" symbol="P398DLP_PULSE_SENSOR_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_PULSE_SENSOR_PKG">
<connects>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="PULSE" pad="PULSE"/>
<connect gate="G$1" pin="VDD" pad="VDD"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_BME680_STEMMA_DEV">
<description>BME680 T/P/RH/VOC STEMMA connector</description>
<gates>
<gate name="STEMMA$1" symbol="P398DLP_BME680_STEMMA_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_BME680_STEMMA_PKG">
<connects>
<connect gate="STEMMA$1" pin="3V0" pad="3VO"/>
<connect gate="STEMMA$1" pin="CS" pad="CS"/>
<connect gate="STEMMA$1" pin="GND" pad="GND"/>
<connect gate="STEMMA$1" pin="SCK" pad="SCK"/>
<connect gate="STEMMA$1" pin="SDI" pad="SDI"/>
<connect gate="STEMMA$1" pin="SDO" pad="SDO"/>
<connect gate="STEMMA$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_2XAA_BATTERY_DEV">
<description>2 x AA battery case</description>
<gates>
<gate name="G$1" symbol="P398DLP_2XAA_BATTERY_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_2XAA_BATTERY_PKG">
<connects>
<connect gate="G$1" pin="BATTERY_3V" pad="BATTERY_3V"/>
<connect gate="G$1" pin="BATTERY_GND" pad="BATTERY_GND"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_SPDT_DIP_SLIDE_SWITCH_DEV">
<description>SPDT slide switch, .098 inch pitch: EG1218 E-SWITCH, Adafruit 805</description>
<gates>
<gate name="G$1" symbol="P398DLP_SPDT_DIP_SLIDE_SWITCH_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_SPDT_DIP_SLIDE_SWITCH_PKG">
<connects>
<connect gate="G$1" pin="PIN1" pad="PIN1"/>
<connect gate="G$1" pin="PIN2" pad="PIN2"/>
<connect gate="G$1" pin="PIN3" pad="PIN3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_MOUNTING_HOLE_300MIL_DEV">
<description>0.3 inch hole</description>
<gates>
<gate name="G$1" symbol="P398DLP_MOUNTING_HOLE_300MIL_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_MOUNTING_HOLE_300MIL_PKG">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_BQ24704_SOLAR_CHARGER_DEV">
<description>Adafruit bq24074 solar power charger: part ID 4755</description>
<gates>
<gate name="G$1" symbol="P398DLP_BQ24074_SOLAR_CHARGER_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_BQ24074_SOLAR_CHARGER_PKG">
<connects>
<connect gate="G$1" pin="CE" pad="CE"/>
<connect gate="G$1" pin="CHG" pad="CHG"/>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GND1" pad="GND1"/>
<connect gate="G$1" pin="GND2" pad="GND2"/>
<connect gate="G$1" pin="ISET" pad="ISET"/>
<connect gate="G$1" pin="LIPO" pad="LIPO"/>
<connect gate="G$1" pin="OUT" pad="OUT"/>
<connect gate="G$1" pin="PGOOD" pad="PGOOD"/>
<connect gate="G$1" pin="THERM" pad="THERM"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_USB_MICRO_BREAKOUT_DEV">
<description>Adafruit 1833 microUSB breakout</description>
<gates>
<gate name="G$1" symbol="P398DLP_USB_MICRO_BREAKOUT_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_USB_MICRO_BREAKOUT_PKG">
<connects>
<connect gate="G$1" pin="5V" pad="5V"/>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="ID" pad="ID"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_MOUNTING_HOLE_250MIL_DEV">
<description>0.25 inch hole</description>
<gates>
<gate name="G$1" symbol="P398DLP_MOUNTING_HOLE_250MIL_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_MOUNTING_HOLE_250MIL_PKG">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_USB_C_BREAKOUT_DEV">
<description>Adafruit 4090 USB-C breakout</description>
<gates>
<gate name="G$1" symbol="P398DLP_USB_C_BREAKOUT_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_USB_C_BREAKOUT_PKG">
<connects>
<connect gate="G$1" pin="CC1" pad="CC1"/>
<connect gate="G$1" pin="CC2" pad="CC2"/>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="SBU1" pad="SBU1"/>
<connect gate="G$1" pin="SBU2" pad="SBU2"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_VOLTMETER_DEV">
<description>Adafruit 2-wire voltmeter</description>
<gates>
<gate name="G$1" symbol="P398DLP_VOLTMETER_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_VOLTMETER_PKG">
<connects>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_ADC_QUAD_I2C_DEV">
<description>ADS1015 quad ADC</description>
<gates>
<gate name="G$1" symbol="P398DLP_ADC_QUAD_I2C_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_ADC_QUAD_I2C_PKG">
<connects>
<connect gate="G$1" pin="A0" pad="A0"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="ADDR" pad="ADDR"/>
<connect gate="G$1" pin="ALRT" pad="ALRT"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="SCL" pad="SCL"/>
<connect gate="G$1" pin="SDA" pad="SDA"/>
<connect gate="G$1" pin="VDD" pad="VDD"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_DPS310_DEV">
<description>DPS310 precision pressure and temperature sensor. Adafruit 4494</description>
<gates>
<gate name="G$1" symbol="P398DLP_DPS310_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_DPS310_PKG">
<connects>
<connect gate="G$1" pin="3VO" pad="3VO"/>
<connect gate="G$1" pin="CS" pad="CS"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="SCK" pad="SCK"/>
<connect gate="G$1" pin="SDI" pad="SDI"/>
<connect gate="G$1" pin="SDO" pad="SDO"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_RIBBON_PCB_2X3_DEV" prefix="PL" uservalue="yes">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="6P"/>
</gates>
<devices>
<device name="" package="06V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_MCP4728_DEV">
<description>MCP4725 12-bit DACMCP4728 quad 12-bit DAC Adafriuit 4470</description>
<gates>
<gate name="G$1" symbol="P398DLP_MCP4728_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_MCP4728_PKG">
<connects>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GND2" pad="GND2"/>
<connect gate="G$1" pin="LDAC" pad="LDAC"/>
<connect gate="G$1" pin="RDY" pad="RDY"/>
<connect gate="G$1" pin="SCL" pad="SCL"/>
<connect gate="G$1" pin="SDA" pad="SDA"/>
<connect gate="G$1" pin="VA" pad="VA"/>
<connect gate="G$1" pin="VB" pad="VB"/>
<connect gate="G$1" pin="VC" pad="VC"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
<connect gate="G$1" pin="VCC2" pad="VCC2"/>
<connect gate="G$1" pin="VD" pad="VD"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_AS7262_DEV">
<description>AS7262 6 channel visible light sensor</description>
<gates>
<gate name="G$1" symbol="P398DLP_AS7262_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_AS7262_PKG">
<connects>
<connect gate="G$1" pin="3V3" pad="3V3"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GND2" pad="GND2"/>
<connect gate="G$1" pin="INT" pad="INT"/>
<connect gate="G$1" pin="LED" pad="LED"/>
<connect gate="G$1" pin="NC1" pad="NC1"/>
<connect gate="G$1" pin="NC2" pad="NC2"/>
<connect gate="G$1" pin="RST" pad="RST"/>
<connect gate="G$1" pin="RX" pad="RX"/>
<connect gate="G$1" pin="SCL" pad="SCL"/>
<connect gate="G$1" pin="SDA" pad="SDA"/>
<connect gate="G$1" pin="TX" pad="TX"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
<connect gate="G$1" pin="VIN2" pad="VIN2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_NPN_DEV">
<description>NPN transistor, TO-92 case</description>
<gates>
<gate name="G$1" symbol="P398DLP_NPN_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_NPN_PKG">
<connects>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$1" pin="E" pad="E"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_SONY_SPRESENSE_EXTENSION_DEV">
<description>Sony Spresense extension board</description>
<gates>
<gate name="G$1" symbol="P398DLP_SONY_SPRESENSE_EXTENSION_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_SONY_SPRESENSE_EXTENSION_PKG">
<connects>
<connect gate="G$1" pin="1.8V2_" pad="1.8V2_"/>
<connect gate="G$1" pin="1.8V_" pad="1.8V_"/>
<connect gate="G$1" pin="3.3V" pad="3.3V"/>
<connect gate="G$1" pin="3.3V1_" pad="3.3V1_"/>
<connect gate="G$1" pin="5V1" pad="5V1"/>
<connect gate="G$1" pin="A0" pad="A0"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A2_" pad="A2_"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A3_" pad="A3_"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="AREF" pad="AREF"/>
<connect gate="G$1" pin="D00-&gt;RX" pad="D00-&gt;RX"/>
<connect gate="G$1" pin="D00_" pad="D00_"/>
<connect gate="G$1" pin="D01&lt;-TX" pad="D01&lt;-TX"/>
<connect gate="G$1" pin="D01_" pad="D01_"/>
<connect gate="G$1" pin="D02" pad="D02"/>
<connect gate="G$1" pin="D03" pad="D03_PWM"/>
<connect gate="G$1" pin="D04" pad="D04"/>
<connect gate="G$1" pin="D05" pad="D05_PWM"/>
<connect gate="G$1" pin="D06" pad="D06_PWM"/>
<connect gate="G$1" pin="D07" pad="D07"/>
<connect gate="G$1" pin="D08" pad="D08"/>
<connect gate="G$1" pin="D09" pad="D09_PWM"/>
<connect gate="G$1" pin="D10" pad="D10_SPI_CS"/>
<connect gate="G$1" pin="D11" pad="D11_SPI_MOSI"/>
<connect gate="G$1" pin="D12" pad="D12_SPI_MISO"/>
<connect gate="G$1" pin="D13" pad="D13_SPI_SCK"/>
<connect gate="G$1" pin="D14" pad="D14_I2C_SDA"/>
<connect gate="G$1" pin="D14_" pad="D14_"/>
<connect gate="G$1" pin="D15" pad="D15_I2C_SCL"/>
<connect gate="G$1" pin="D15_" pad="D15_"/>
<connect gate="G$1" pin="D16_" pad="D16_"/>
<connect gate="G$1" pin="D17_" pad="D17_"/>
<connect gate="G$1" pin="D18_" pad="D18_"/>
<connect gate="G$1" pin="D19_" pad="D19_"/>
<connect gate="G$1" pin="D20_" pad="D20_"/>
<connect gate="G$1" pin="D21_" pad="D21_"/>
<connect gate="G$1" pin="D22_" pad="D22_"/>
<connect gate="G$1" pin="D23_" pad="D23_"/>
<connect gate="G$1" pin="D24_" pad="D24_"/>
<connect gate="G$1" pin="D25_" pad="D25_"/>
<connect gate="G$1" pin="D26_" pad="D26_"/>
<connect gate="G$1" pin="D27_" pad="D27_"/>
<connect gate="G$1" pin="D28_" pad="D28_"/>
<connect gate="G$1" pin="EXT_VDD" pad="EXT_VDD"/>
<connect gate="G$1" pin="GND1" pad="GND1"/>
<connect gate="G$1" pin="GND2" pad="GND2"/>
<connect gate="G$1" pin="GND3" pad="GND3"/>
<connect gate="G$1" pin="GND4_" pad="GND4_"/>
<connect gate="G$1" pin="GND5_" pad="GND5_"/>
<connect gate="G$1" pin="IOREF" pad="IOREF"/>
<connect gate="G$1" pin="RESERVE1" pad="NC"/>
<connect gate="G$1" pin="RESERVE2" pad="NC2"/>
<connect gate="G$1" pin="RESET" pad="RESET"/>
<connect gate="G$1" pin="XRST_PIN_1.8V" pad="XRST_PIN_1.8V"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_MLX90640_CAMERA_DEV">
<description>MLX90640 low resolution IR camera. Adafruit 4407</description>
<gates>
<gate name="G$1" symbol="P398DLP_MLX90640_CAMERA_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_MLX90640_CAMERA_PKG">
<connects>
<connect gate="G$1" pin="3VO" pad="3VO"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="SCL" pad="SCL"/>
<connect gate="G$1" pin="SDA" pad="SDA"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_RED_LED_DEV" prefix="JP" uservalue="yes">
<description>red LED</description>
<gates>
<gate name="G$1" symbol="P398DLP_RED_LED_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_RED_LED_PKG">
<connects>
<connect gate="G$1" pin="NEG" pad="NEG"/>
<connect gate="G$1" pin="POS" pad="POS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_ROTARY_SWITCH_DEV">
<description>CTSCORP.com rotary switch
220ADC16</description>
<gates>
<gate name="G$1" symbol="P398DLP_ROTARY_SWITCH_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_ROTARY_SWITCH_PKG">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="C1" pad="C1"/>
<connect gate="G$1" pin="C2" pad="C2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_ROSE4_DEV">
<description>rose bitmap</description>
<gates>
<gate name="G$1" symbol="P398DLP_ROSE4_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_ROSE4_PKG">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_TFT_DISPLAY_DEV">
<description>160x128 TFT display</description>
<gates>
<gate name="G$1" symbol="P398DLP_TFT_DISPLAY_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_TFT_DISPLAY_PKG">
<connects>
<connect gate="G$1" pin="CARD_CS" pad="CARD_CS"/>
<connect gate="G$1" pin="D/C" pad="D/C"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="LITE" pad="LITE"/>
<connect gate="G$1" pin="MISO" pad="MISO"/>
<connect gate="G$1" pin="MOSI" pad="MOSI"/>
<connect gate="G$1" pin="RESET" pad="RESET"/>
<connect gate="G$1" pin="SCK" pad="SCK"/>
<connect gate="G$1" pin="TFT_CS" pad="TFT_CS"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_LC709203F_STEMMA_DEV">
<description>LC709203F LiPo "fuel gauge"</description>
<gates>
<gate name="G$1" symbol="P398DLP_LC709203F_STEMMA_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_LC709203F_STEMMA_PKG">
<connects>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="INT" pad="INT"/>
<connect gate="G$1" pin="SCL" pad="SCL"/>
<connect gate="G$1" pin="SDA" pad="SDA"/>
<connect gate="G$1" pin="THERM" pad="THERM"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_PUSHBUTTON2A_DEV">
<description>pushbutton</description>
<gates>
<gate name="G$1" symbol="P398DLP_PUSHBUTTON2A_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_PUSHBUTTON2A_PKG">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$1" pin="D" pad="D"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_AS7341_DEV">
<description>AS7341 10 channel spectrometer</description>
<gates>
<gate name="G$1" symbol="P398DLP_AS7341_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_AS7341_PKG">
<connects>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GPIO" pad="GPIO"/>
<connect gate="G$1" pin="INT" pad="INT"/>
<connect gate="G$1" pin="SCL" pad="SCL"/>
<connect gate="G$1" pin="SDA" pad="SDA"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_PHOTO_INTERRUPTER_DEV">
<description>Adafruit four-wire photo interrupter</description>
<gates>
<gate name="G$1" symbol="P398DLP_PHOTO_INTERRUPTER_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_PHOTO_INTERRUPTER_PKG">
<connects>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="LED" pad="LED"/>
<connect gate="G$1" pin="OUT" pad="OUTPUT"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_SFM3300_HEADER_DEV">
<description>Sensirion SFM3300 flowmeter header</description>
<gates>
<gate name="G$1" symbol="P398DLP_SFM3300_HEADER_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_SFM3300_HEADER_PKG">
<connects>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="HEAT" pad="HEAT"/>
<connect gate="G$1" pin="HEAT_GND" pad="HEAT_GND"/>
<connect gate="G$1" pin="SCK" pad="SCK"/>
<connect gate="G$1" pin="SDA" pad="SDA"/>
<connect gate="G$1" pin="VDD" pad="VDD"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_DC_DC_CONVERTER_DEV">
<description>RECOM ROE SIP4 DC-DC converter
3,3 V to 5 V
ROE-3..305S part number</description>
<gates>
<gate name="G$1" symbol="P398DLP_DC_DC_CONVERTER_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_DC_DC_CONVERTER_PKG">
<connects>
<connect gate="G$1" pin="NEG_VIN" pad="NEG_VIN"/>
<connect gate="G$1" pin="NEG_VOUT" pad="NEG_VOUT"/>
<connect gate="G$1" pin="POS_VIN" pad="POS_VIN"/>
<connect gate="G$1" pin="POS_VOUT" pad="POS_VOUT"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_L4931_REG_DEV">
<description>L4931 linear voltage regulator, TO-92 case 5.0V, adafruit 2236</description>
<gates>
<gate name="G$1" symbol="P398DLP_L4931_REG_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_L4931_REG_PKG">
<connects>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
<connect gate="G$1" pin="VOUT" pad="VOUT"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_MAX30102_SPARKFUN_DEV">
<description>SparkFun Max30102 board
P398DLP_MAX30102_SPARKFUN</description>
<gates>
<gate name="G$1" symbol="P398DLP_MAX30102_SPARKFUN_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_MAX30102_SPARKFUN_PKG">
<connects>
<connect gate="G$1" pin="3V3_BOT" pad="3V3_BOT"/>
<connect gate="G$1" pin="3V3_TOP" pad="3V3_TOP"/>
<connect gate="G$1" pin="GND_BOT" pad="GND_BOT"/>
<connect gate="G$1" pin="GND_TOP" pad="GND_TOP"/>
<connect gate="G$1" pin="SCL_BOT" pad="SCL_BOT"/>
<connect gate="G$1" pin="SCL_TOP" pad="SCL_TOP"/>
<connect gate="G$1" pin="SDA_BOT" pad="SDA_BOT"/>
<connect gate="G$1" pin="SDA_TOP" pad="SDA_TOP"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_ADXL375_DEV">
<description>ADXL375 200 g accelerometer</description>
<gates>
<gate name="G$1" symbol="P398DLP_ADXL375_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_ADXL375_PKG">
<connects>
<connect gate="G$1" pin="3VO" pad="3VO"/>
<connect gate="G$1" pin="CS" pad="CS"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GND2" pad="GND2"/>
<connect gate="G$1" pin="I2" pad="I2"/>
<connect gate="G$1" pin="INT" pad="INT"/>
<connect gate="G$1" pin="SCL" pad="SCL"/>
<connect gate="G$1" pin="SDA" pad="SDA"/>
<connect gate="G$1" pin="SDO" pad="SDO"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P398DLP_H3LIS331_DEV">
<description>H3LIS331 400 g accelerometer</description>
<gates>
<gate name="G$1" symbol="P398DLP_H3LIS331_SYM"/>
</gates>
<devices>
<device name="" package="P398DLP_H3LIS331_PKG">
<connects>
<connect gate="G$1" pin="3VO" pad="3VO"/>
<connect gate="G$1" pin="CS" pad="CS"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="I2" pad="I2"/>
<connect gate="G$1" pin="INT" pad="INT"/>
<connect gate="G$1" pin="NC1" pad="NC1"/>
<connect gate="G$1" pin="NC2" pad="NC2"/>
<connect gate="G$1" pin="NC3" pad="NC3"/>
<connect gate="G$1" pin="SCL" pad="SCL"/>
<connect gate="G$1" pin="SDA" pad="SDA"/>
<connect gate="G$1" pin="SDO" pad="SDO"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
