<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="160" y2="0" width="0" layer="20"/>
<wire x1="160" y1="0" x2="160" y2="111.43" width="0" layer="20"/>
<wire x1="160" y1="111.43" x2="0" y2="111.43" width="0" layer="20"/>
<wire x1="0" y1="111.43" x2="0" y2="0" width="0" layer="20"/>
<text>Group 2 - "The Mighty Ducks"
PHYS371 - Spring 2023
Barrus, Coady, Tort Serrataco
Vazquez, Pazhani
PCB v1.0
</text>
<text>Arduino Mega 2560</text>
<text>Distance Sensor
VL53L0X</text>
<text>MicroSD </text>
<text>Laser Emitter 1</text>
<text>Laser Receiver 1</text>
<text>Laser Receiver 2</text>
<text>Laser Emitter 2</text>
<text>Arducam Mini</text>
<text>TFT Display </text>
<text>JLCJLCJLCJLC</text>
<text>Designed by M.Hoppesch
1 March 2023</text>
<text>Project in collaboration w/
the UIUC NPL ATLAS Heavy Ion
Group - Hoppesch &amp; Longo </text>
</plain>
<libraries>
<library name="GDG_library">
<packages>
<package name="GDG_ARDUINO_MEGA2560_PKG">
<description>Arduino MEGA 2560, component side DOWN</description>
</package>
<package name="GDG_MICROSD_PKG">
<description>Adafruit microSD reader breakout board</description>
</package>
<package name="GDG_TFT_DISPLAY_PKG">
<description>160x128 TFT display</description>
</package>
</packages>
</library>
<library name="RL_library">
<packages>
<package name="LB135_LASER_RECEIVER">
<description>LB135 LASER RECEIVER - it reads out the signal sent by the LB135 LASER TRANSMITTER</description>
</package>
</packages>
</library>
<library name="p398dlp">
<packages>
<package name="P398DLP_5XAA_BATTERY_PKG">
<description>Adafruit 5 x AA battery pack</description>
</package>
<package name="P398DLP_VL53L0X_PKG">
<description>VL53L0X proximity sensor</description>
</package>
<package name="P398DLP_1N5817_PKG">
<description>1N5817 Schottky barrier diode</description>
</package>
<package name="P398DLP_MOUNTING_HOLE_4MM_PKG">
</package>
</packages>
</library>
<library name="SparkFun-Sensors">
<description>&lt;h3&gt;SparkFun Sensors&lt;/h3&gt;
This library contains sensors- accelerometers, gyros, compasses, magnetometers, light sensors, imagers, temp sensors, etc.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application.
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TO-92-AMMO">
<description>&lt;h3&gt;TO-92 3-Pin PTH AMMO package&lt;/h3&gt;
&lt;p&gt;&lt;a href=""&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;
&lt;li&gt;Pin Count: 3&lt;/li&gt;
&lt;li&gt;Dimensions:  3.68 x 4.83 x 4.83 mm&lt;/li&gt;
&lt;li&gt;Pitch: 2.54 mm&lt;/li&gt;
&lt;/ul&gt;
&lt;p&gt;Devices Using:&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;DS18B20&lt;/li&gt;
&lt;/ul&gt;</description>
</package>
</packages>
</library>
<library name="RL_library (1)">
<packages>
<package name="ARDUCAM_MINI">
<description>ARDUCAM MINI</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="GDG_library" package="GDG_ARDUINO_MEGA2560_PKG" value="GDG_ARDUINO_MEGA2560_DEV"/>
<element name="U$2" library="GDG_library" package="GDG_MICROSD_PKG" value="GDG_MICROSD_DEV"/>
<element name="U$4" library="RL_library" package="LB135_LASER_RECEIVER" value="LB135_LASER_RECEIVER"/>
<element name="U$5" library="RL_library" package="LB135_LASER_RECEIVER" value="LB135_LASER_RECEIVER"/>
<element name="U$6" library="GDG_library" package="GDG_TFT_DISPLAY_PKG" value="GDG_TFT_DISPLAY_DEV"/>
<element name="U$7" library="p398dlp" package="P398DLP_5XAA_BATTERY_PKG" value="P398DLP_5XAA_BATTERY_DEV"/>
<element name="U$8" library="p398dlp" package="P398DLP_VL53L0X_PKG" value="P398DLP_VL53L0X_DEV"/>
<element name="U$9" library="p398dlp" package="P398DLP_1N5817_PKG" value="P398DLP_1N5817_DEV">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="SparkFun-Sensors" package="TO-92-AMMO" value="DS18B20">
<attribute name="NAME"/>
<attribute name="STORE_ID" value="SEN-00245"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="SparkFun-Sensors" package="TO-92-AMMO" value="DS18B20">
<attribute name="NAME"/>
<attribute name="STORE_ID" value="SEN-00245"/>
<attribute name="VALUE"/>
</element>
<element name="U$10" library="p398dlp" package="P398DLP_MOUNTING_HOLE_4MM_PKG" value=""/>
<element name="U$11" library="p398dlp" package="P398DLP_MOUNTING_HOLE_4MM_PKG" value=""/>
<element name="U$12" library="p398dlp" package="P398DLP_MOUNTING_HOLE_4MM_PKG" value=""/>
<element name="U$13" library="p398dlp" package="P398DLP_MOUNTING_HOLE_4MM_PKG" value=""/>
<element name="U$14" library="RL_library (1)" package="ARDUCAM_MINI" value="ARDUCAM_MINI"/>
</elements>
<signals>
<signal name="GND">
<contactref element="U$1" pad="GND2"/>
<contactref element="U$2" pad="3"/>
<contactref element="U$5" pad="P$1"/>
<contactref element="U$4" pad="P$1"/>
<contactref element="U1" pad="1"/>
<contactref element="U2" pad="1"/>
<contactref element="U$6" pad="GND"/>
<contactref element="U$8" pad="GND"/>
<contactref element="U$7" pad="BATTERY_GND"/>
<contactref element="U$14" pad="GND"/>
</signal>
<signal name="5V">
<contactref element="U$1" pad="5V1"/>
<contactref element="U$2" pad="1"/>
<contactref element="U1" pad="3"/>
<contactref element="U2" pad="3"/>
<contactref element="U$5" pad="P$3"/>
<contactref element="U$4" pad="P$3"/>
<contactref element="U$6" pad="VCC"/>
<contactref element="U$8" pad="VIN"/>
<contactref element="U$9" pad="C"/>
<contactref element="U$14" pad="VCC"/>
</signal>
<signal name="CLK">
<contactref element="U$2" pad="4"/>
<contactref element="U$1" pad="D53"/>
</signal>
<signal name="DO">
<contactref element="U$2" pad="5"/>
<contactref element="U$1" pad="D51"/>
</signal>
<signal name="DI">
<contactref element="U$2" pad="6"/>
<contactref element="U$1" pad="D52"/>
</signal>
<signal name="CS">
<contactref element="U$2" pad="7"/>
<contactref element="U$1" pad="D50"/>
</signal>
<signal name="DQ2">
<contactref element="U$1" pad="D2"/>
<contactref element="U2" pad="2"/>
</signal>
<signal name="DQ1">
<contactref element="U$1" pad="D3"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="SCL">
<contactref element="U$1" pad="D21SCL"/>
<contactref element="U$8" pad="SCL"/>
<contactref element="U$14" pad="SCL"/>
</signal>
<signal name="SDA">
<contactref element="U$1" pad="D20SDA"/>
<contactref element="U$8" pad="SDA"/>
<contactref element="U$14" pad="SDA"/>
</signal>
<signal name="SCK">
<contactref element="U$1" pad="D27"/>
<contactref element="U$14" pad="SCK"/>
</signal>
<signal name="MISO">
<contactref element="U$1" pad="D29"/>
<contactref element="U$14" pad="MISO"/>
</signal>
<signal name="MOSI">
<contactref element="U$1" pad="D31"/>
<contactref element="U$14" pad="MOSI"/>
</signal>
<signal name="LASER_OUT">
<contactref element="U$1" pad="D35"/>
<contactref element="U$5" pad="P$2"/>
</signal>
<signal name="LASER_OUT2">
<contactref element="U$1" pad="D37"/>
<contactref element="U$4" pad="P$2"/>
</signal>
<signal name="TFT_CCS">
<contactref element="U$1" pad="D6"/>
<contactref element="U$6" pad="CARD_CS"/>
</signal>
<signal name="TFT_TCS">
<contactref element="U$1" pad="D5"/>
<contactref element="U$6" pad="TFT_CS"/>
</signal>
<signal name="TFT_DC">
<contactref element="U$1" pad="D41"/>
<contactref element="U$6" pad="D/C"/>
</signal>
<signal name="TFT_SCK">
<contactref element="U$1" pad="D43"/>
<contactref element="U$6" pad="SCK"/>
</signal>
<signal name="TFT_SO">
<contactref element="U$1" pad="D45"/>
<contactref element="U$6" pad="MISO"/>
</signal>
<signal name="TFT_SI">
<contactref element="U$1" pad="D47"/>
<contactref element="U$6" pad="MOSI"/>
</signal>
<signal name="N$5">
<contactref element="U$9" pad="A"/>
<contactref element="U$7" pad="BATTERY_7.5V"/>
</signal>
<signal name="CS_D7">
<contactref element="U$1" pad="D7"/>
<contactref element="U$14" pad="CS"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
