<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="-5.08" x2="134.6" y2="-5.08" width="0" layer="20"/>
<wire x1="134.6" y1="-5.08" x2="134.6" y2="98.73" width="0" layer="20"/>
<wire x1="134.6" y1="98.73" x2="0" y2="98.73" width="0" layer="20"/>
<wire x1="0" y1="98.73" x2="0" y2="-5.08" width="0" layer="20"/>
<text>Group 3 - "The Froggers"
PHYS371 - Spring 2023
Bender,Glasheen, Hsu,
Hung, Jain
PCB v1.0</text>
<text>JLCJLCJLCJLC</text>
<text>Designed on 27th Feb 2023</text>
</plain>
<libraries>
<library name="GDG_library">
<packages>
<package name="GDG_ARDUINO_MEGA2560_PKG">
<description>Arduino MEGA 2560, component side DOWN</description>
</package>
<package name="GDG_BME680_PKG">
<description>BME680 temperature, pressure, relative humidity, and volatile organic compounds sensor</description>
</package>
<package name="GDG_5XAA_BATTERY_PKG">
<description>Adafruit 5 x AA battery pack</description>
</package>
<package name="GDG_GP2Y0A21YK0F_IR_PROXIMITY_PKG">
<description>IR proximity sensor</description>
</package>
<package name="GDG_DS3231_PKG">
<description>DS3231 real time clock with battery backup</description>
</package>
<package name="GDG_MICROSD_PKG">
<description>Adafruit microSD reader breakout board</description>
</package>
<package name="GDG_MOUNTING_HOLE_4MM_PKG">
</package>
</packages>
</library>
<library name="RL_library">
<packages>
<package name="ARDUCAM_MINI">
<description>ARDUCAM MINI</description>
</package>
</packages>
</library>
<library name="capacitor-wima">
<description>&lt;b&gt;WIMA Capacitors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="C5B5">
<description>&lt;B&gt;MKS2&lt;/B&gt;, 7.5 x 5 mm, grid 5.08 mm</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="GDG_library" package="GDG_ARDUINO_MEGA2560_PKG" value="GDG_ARDUINO_MEGA2560_DEV"/>
<element name="U$2" library="RL_library" package="ARDUCAM_MINI" value=""/>
<element name="U$3" library="GDG_library" package="GDG_BME680_PKG" value="GDG_BME680_DEV"/>
<element name="U$4" library="GDG_library" package="GDG_5XAA_BATTERY_PKG" value="GDG_5XAA_BATTERY_DEV"/>
<element name="U$5" library="GDG_library" package="GDG_GP2Y0A21YK0F_IR_PROXIMITY_PKG" value="GDG_GP2Y0A21YK0F_IR_PROXIMITY_DEV"/>
<element name="U$6" library="GDG_library" package="GDG_GP2Y0A21YK0F_IR_PROXIMITY_PKG" value="GDG_GP2Y0A21YK0F_IR_PROXIMITY_DEV"/>
<element name="U$7" library="GDG_library" package="GDG_DS3231_PKG" value="GDG_DS3231_DEV"/>
<element name="U$8" library="GDG_library" package="GDG_MICROSD_PKG" value="GDG_MICROSD_DEV"/>
<element name="C_BME" library="capacitor-wima" package="C5B5" value="0.1uF">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="1"/>
<attribute name="VALUE"/>
</element>
<element name="U$9" library="GDG_library" package="GDG_MOUNTING_HOLE_4MM_PKG" value=""/>
<element name="U$10" library="GDG_library" package="GDG_MOUNTING_HOLE_4MM_PKG" value=""/>
<element name="U$11" library="GDG_library" package="GDG_MOUNTING_HOLE_4MM_PKG" value=""/>
<element name="U$12" library="GDG_library" package="GDG_MOUNTING_HOLE_4MM_PKG" value=""/>
</elements>
<signals>
<signal name="5V">
<contactref element="U$1" pad="5V1"/>
<contactref element="U$3" pad="1"/>
<contactref element="U$5" pad="5V"/>
<contactref element="U$6" pad="5V"/>
<contactref element="U$2" pad="VCC"/>
<contactref element="U$7" pad="1"/>
<contactref element="U$8" pad="1"/>
<contactref element="C_BME" pad="2"/>
</signal>
<signal name="GND">
<contactref element="U$3" pad="3"/>
<contactref element="U$5" pad="IR_PROXIMITY"/>
<contactref element="U$6" pad="IR_PROXIMITY"/>
<contactref element="U$7" pad="2"/>
<contactref element="U$2" pad="GND"/>
<contactref element="U$8" pad="3"/>
<contactref element="U$1" pad="GND1"/>
<contactref element="C_BME" pad="1"/>
</signal>
<signal name="I2C_SCL">
<contactref element="U$3" pad="4"/>
<contactref element="U$2" pad="SCL"/>
<contactref element="U$7" pad="3"/>
<contactref element="U$1" pad="D21SCL"/>
</signal>
<signal name="I2C_SDA">
<contactref element="U$3" pad="6"/>
<contactref element="U$2" pad="SDA"/>
<contactref element="U$7" pad="4"/>
<contactref element="U$1" pad="D20SDA"/>
</signal>
<signal name="DI_6">
<contactref element="U$5" pad="GND"/>
<contactref element="U$1" pad="D6"/>
</signal>
<signal name="DI_5">
<contactref element="U$6" pad="GND"/>
<contactref element="U$1" pad="D5"/>
</signal>
<signal name="DI_7">
<contactref element="U$2" pad="CS"/>
<contactref element="U$1" pad="D7"/>
</signal>
<signal name="SPI_CLK">
<contactref element="U$8" pad="4"/>
<contactref element="U$1" pad="D52"/>
</signal>
<signal name="SPI_DO">
<contactref element="U$8" pad="5"/>
<contactref element="U$1" pad="D51"/>
</signal>
<signal name="SPI_DI">
<contactref element="U$8" pad="6"/>
<contactref element="U$1" pad="D50"/>
</signal>
<signal name="SPI_CS">
<contactref element="U$8" pad="7"/>
<contactref element="U$1" pad="D53"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
