<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="-31.75" x2="160" y2="-31.75" width="0" layer="20"/>
<wire x1="160" y1="-31.75" x2="160" y2="122.86" width="0" layer="20"/>
<wire x1="160" y1="122.86" x2="0" y2="122.86" width="0" layer="20"/>
<wire x1="0" y1="122.86" x2="0" y2="-31.75" width="0" layer="20"/>
<text>Group 5 - "The Big Wave"
PHYS371 - Spring 2023
Friar, Howard, Luebbers
Schultz, Wlodarczyk
PCB v1.0</text>
<text>MUX</text>
<text>RTC</text>
<text>Micro SD reader</text>
<text>LCD</text>
<text>Trimpot</text>
<text>Arduino Mega 2560</text>
<text>Accelerometer-CTRL</text>
<text>Accelerometer-1</text>
<text>Accelerometer-2</text>
<text>Accelerometer-3</text>
<text>Accelerometer-4</text>
<text>Designed on 24th Feb 2023</text>
<text>JLCJLCJLCJLC</text>
</plain>
<libraries>
<library name="capacitor-wima">
<description>&lt;b&gt;WIMA Capacitors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="C5B5">
<description>&lt;B&gt;MKS2&lt;/B&gt;, 7.5 x 5 mm, grid 5.08 mm</description>
</package>
</packages>
</library>
<library name="GDG_library">
<packages>
<package name="GDG_ARDUINO_MEGA2560_PKG">
<description>Arduino MEGA 2560, component side DOWN</description>
</package>
<package name="GDG_LCD_16X2_PKG">
<description>2x16 liquid crystal display, four mounting holes. Crystalfontz CFAH1602B-NGG-JTV</description>
</package>
<package name="GDG_5XAA_BATTERY_PKG">
<description>Adafruit 5 x AA battery pack</description>
</package>
<package name="GDG_TRIMPOT_PKG">
<description>trimpot</description>
</package>
<package name="GDG_DS3231_PKG">
<description>DS3231 real time clock with battery backup</description>
</package>
<package name="GDG_MICROSD_PKG">
<description>Adafruit microSD reader breakout board</description>
</package>
<package name="GDG_TCA9548A_MUX_PKG">
<description>TCA9548A I2C MUX</description>
</package>
<package name="GDG_LSM9DS1_9DOF_PKG">
<description>LSM9DS1 accelerometer, gyroscope, magnetometer</description>
</package>
<package name="GDG_MOUNTING_HOLE_4MM_PKG">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C_LCD" library="capacitor-wima" package="C5B5" value="0.1uF">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="1"/>
<attribute name="VALUE"/>
</element>
<element name="C_SD" library="capacitor-wima" package="C5B5" value="0.1uF">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="1"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="GDG_library" package="GDG_ARDUINO_MEGA2560_PKG" value="GDG_ARDUINO_MEGA2560_DEV"/>
<element name="U$10" library="GDG_library" package="GDG_LCD_16X2_PKG" value="GDG_LCD_16X2_DEV"/>
<element name="U$12" library="GDG_library" package="GDG_5XAA_BATTERY_PKG" value="GDG_5XAA_BATTERY_DEV"/>
<element name="U$13" library="GDG_library" package="GDG_TRIMPOT_PKG" value="GDG_TRIMPOT_DEV">
<attribute name="VALUE"/>
</element>
<element name="U$2" library="GDG_library" package="GDG_DS3231_PKG" value="GDG_DS3231_DEV"/>
<element name="U$3" library="GDG_library" package="GDG_MICROSD_PKG" value="GDG_MICROSD_DEV"/>
<element name="U$4" library="GDG_library" package="GDG_TCA9548A_MUX_PKG" value="GDG_TCA9548A_MUX_DEV"/>
<element name="U$5" library="GDG_library" package="GDG_LSM9DS1_9DOF_PKG" value="GDG_LSM9DS1_9DOF_DEVLSM"/>
<element name="U$6" library="GDG_library" package="GDG_LSM9DS1_9DOF_PKG" value="GDG_LSM9DS1_9DOF_DEVLSM"/>
<element name="U$7" library="GDG_library" package="GDG_LSM9DS1_9DOF_PKG" value="GDG_LSM9DS1_9DOF_DEVLSM"/>
<element name="U$8" library="GDG_library" package="GDG_LSM9DS1_9DOF_PKG" value="GDG_LSM9DS1_9DOF_DEVLSM"/>
<element name="U$9" library="GDG_library" package="GDG_LSM9DS1_9DOF_PKG" value="GDG_LSM9DS1_9DOF_DEVLSM"/>
<element name="U$11" library="GDG_library" package="GDG_MOUNTING_HOLE_4MM_PKG" value=""/>
<element name="U$14" library="GDG_library" package="GDG_MOUNTING_HOLE_4MM_PKG" value=""/>
<element name="U$15" library="GDG_library" package="GDG_MOUNTING_HOLE_4MM_PKG" value=""/>
<element name="U$16" library="GDG_library" package="GDG_MOUNTING_HOLE_4MM_PKG" value=""/>
</elements>
<signals>
<signal name="VIN">
<contactref element="U$4" pad="VIN"/>
<contactref element="U$1" pad="5V1"/>
<contactref element="U$2" pad="1"/>
<contactref element="U$3" pad="1"/>
<contactref element="C_SD" pad="1"/>
<contactref element="U$5" pad="VIN"/>
<contactref element="U$6" pad="VIN"/>
<contactref element="U$7" pad="VIN"/>
<contactref element="U$8" pad="VIN"/>
<contactref element="U$9" pad="VIN"/>
<contactref element="U$10" pad="5V"/>
<contactref element="C_LCD" pad="1"/>
<contactref element="U$13" pad="BOTTOM"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="GND1"/>
<contactref element="U$4" pad="GND"/>
<contactref element="U$10" pad="GND"/>
<contactref element="U$10" pad="R/W"/>
<contactref element="C_LCD" pad="2"/>
<contactref element="U$9" pad="GND"/>
<contactref element="U$8" pad="GND"/>
<contactref element="U$7" pad="GND"/>
<contactref element="U$6" pad="GND"/>
<contactref element="U$3" pad="3"/>
<contactref element="C_SD" pad="2"/>
<contactref element="U$5" pad="GND"/>
<contactref element="U$2" pad="2"/>
</signal>
<signal name="SDCS">
<contactref element="U$1" pad="D53"/>
<contactref element="U$3" pad="7"/>
</signal>
<signal name="SDDI">
<contactref element="U$1" pad="D51"/>
<contactref element="U$3" pad="6"/>
</signal>
<signal name="SDDO">
<contactref element="U$1" pad="D50"/>
<contactref element="U$3" pad="5"/>
</signal>
<signal name="SDCLK">
<contactref element="U$1" pad="D52"/>
<contactref element="U$3" pad="4"/>
</signal>
<signal name="SDA">
<contactref element="U$1" pad="D20SDA"/>
<contactref element="U$2" pad="4"/>
<contactref element="U$4" pad="SDA"/>
</signal>
<signal name="SCL">
<contactref element="U$1" pad="D21SCL"/>
<contactref element="U$2" pad="3"/>
<contactref element="U$4" pad="SCL"/>
</signal>
<signal name="SC1">
<contactref element="U$4" pad="SC1"/>
<contactref element="U$5" pad="SCL"/>
</signal>
<signal name="SD1">
<contactref element="U$4" pad="SD1"/>
<contactref element="U$5" pad="SDA"/>
</signal>
<signal name="SC7">
<contactref element="U$4" pad="SC7"/>
<contactref element="U$6" pad="SCL"/>
</signal>
<signal name="SD7">
<contactref element="U$4" pad="SD7"/>
<contactref element="U$6" pad="SDA"/>
</signal>
<signal name="SC6">
<contactref element="U$4" pad="SC6"/>
<contactref element="U$7" pad="SCL"/>
</signal>
<signal name="SD6">
<contactref element="U$4" pad="SD6"/>
<contactref element="U$7" pad="SDA"/>
</signal>
<signal name="SC5">
<contactref element="U$4" pad="SC5"/>
<contactref element="U$8" pad="SCL"/>
</signal>
<signal name="SD5">
<contactref element="U$4" pad="SD5"/>
<contactref element="U$8" pad="SDA"/>
</signal>
<signal name="SC4">
<contactref element="U$4" pad="SC4"/>
<contactref element="U$9" pad="SCL"/>
</signal>
<signal name="SD4">
<contactref element="U$4" pad="SD4"/>
<contactref element="U$9" pad="SDA"/>
</signal>
<signal name="V0">
<contactref element="U$13" pad="TAP"/>
<contactref element="U$10" pad="VO"/>
</signal>
<signal name="LCDRS">
<contactref element="U$10" pad="RS"/>
<contactref element="U$1" pad="D12"/>
</signal>
<signal name="LCDE">
<contactref element="U$1" pad="D11"/>
<contactref element="U$10" pad="E"/>
</signal>
<signal name="LCDDB4">
<contactref element="U$1" pad="D36"/>
<contactref element="U$10" pad="DB4"/>
</signal>
<signal name="LCDDB5">
<contactref element="U$1" pad="D34"/>
<contactref element="U$10" pad="DB5"/>
</signal>
<signal name="LCDDB6">
<contactref element="U$1" pad="D32"/>
<contactref element="U$10" pad="DB6"/>
</signal>
<signal name="LCDDB7">
<contactref element="U$1" pad="D30"/>
<contactref element="U$10" pad="DB7"/>
</signal>
<signal name="POTOUT">
<contactref element="U$10" pad="PULL"/>
<contactref element="U$13" pad="TOP"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
